For 1990-2009 cars

Table 1: | Underhood Fuse Block (UHFB) Maxifuses
Table 2: | Underhood Fuse Block Minifuses
Table 3: | Underhood Fuse Block Relays
Table 4: | Instrument Panel Fuse Block Minifuses
Table 5: | Instrument Panel Fuse Block Relays/Modules

The wiring circuits in your vehicle are protected from short circuits by fuses. This greatly reduces the chance of circuit overload and fires caused by electrical problems.

There are two fuse blocks in your Saturn vehicle -- the "underhood fuse block" and the "instrument panel fuse block." These fuse blocks are used to identify and check fuses and relays. Refer to the Fuse and Relay Usage Chart inside the fuse panel cover to identify the fuses and relays.

### Instrument Panel Fuse Block

The instrument panel fuse block is located near the passenger's left leg. To remove the fuse panel cover and access the fuses and relays, loosen the screw on the cover and remove the cover.

Refer to the Fuse and Relay Usage Chart on the inside of the fuse panel cover to identify the fuses and relays.

### Underhood Fuse Block

The underhood fuse block is located in the forward part of the engine compartment near the battery. Six spare minifuses and a fuse-puller are located in the fuse block.

To identify and check fuses and relays, refer to the Fuse and relay Usage Chart. To remove a fuse, place the wide end of the fuse puller over the plastic end of the fuse. Squeeze the ends over the fuse and pull the fuse straight out. Do not wiggle or pry fuse out.

Check the fuse by looking at the silver-colored band inside the fuse. If the band is broken or melted, replace the fuse. Be sure you replace a bad fuse with a new one of the same amperage.

You can use a spare minifuse from the underhood fuse block to replace a bad minifuse in either the underhood or instrument panel fuse dlock. Remember to replace spare fuses as they are used as soon as you can.

The following chart lists the maxifuses, located in the underhood fuse block, and the minifuses or the system they control.

Note: A label is provided on the fuse block cover for fuse layout.

#### Underhood Fuse Block (UHFB) Maxifuses

FUSE | COLOR (AMP) | MINIFUSE (AMP) OR SYSTEM
--- | --- | ---
ABS | Red (50) | Anti-Lock Brake System
AIR PUMP | Green (30) | Feeds Directly to AIR PUMP Relay
COOLING FAN | Green (30) | Feeds Directly to COOL FAN Relay (for engine cooling system)
IGN 1/4 | Green (30) | IGN 1 (10), TURN (10), B/U LP (10), EMISS (10), EIS (10), PC I (10), INJ (10), WIPER (25), AIR BAG (10), RADIO (IGN) (10), CRUISE (10), WINDOW Relay, A/C Relay, AIR PUMP Relay
IGN 3 | Green (30) | IGN 3 (10), HVAC (15)
IP BATT | Green (30) | Feeds directly to FUEL PUMP Relay. After relay, FUEL PUMP (10), TRS 3/4 (10), TRS 2/TCC (10), TRS LP (10)
WINDOW | Green (30) | Feeds directly to WINDOW Relay. SUN (15), after WINDOW Relay

The following chart lists the minifuses, located in the underhood fuse block, and the system they control.

Note: A label is provided on the fuse block cover for relay layout.

#### Underhood Fuse Block Minifuses

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
A/C | Red (10) | Air Conditioning (Feeds directly to A/C Relay)
BRAKE | Blue (15) | Brake Lamps
B/U LP | Red (10) | Backup Lamps, Coolant Level Switch
EIS | Red (10) | Electronic Ignition System
EMISS | Red (10) | Exhaust Air Valve Solenoid, Evaporative Emission Canister Purge Solenoid, Rear Oxygen Sensor
FOG LP | Red (10) | Fog Lamps (Feeds directly to FOG LAMP Relay)
HAZARD | Red (10) | Hazard Flasher, Instrument Panel Turn Signal/Lane Change Indicators, Front Park/Turn Lamps, Rear Taillamps
HORN | Red (10) | Horn (Feeds directly to HORN Relay)
INJ | Red (10) | Fuel Injectors
L HDLP | Red (10) | Left Headlamps
PARK LP | Red (10) | Front Park Lamps, Front Marker Lamps, Fog Lamps, Rear Tail Lamps, License Plate Lamps, Backlight Dimming for Instrument Panel, Radio Display, Climate Control Module, PRND32 Shifter Indicator
PCM B | Red (10) | Powertrain Control Module Memory
PCM I | Red (10) | Powertrain Control Module
R HDLP | Red (10) | Right Headlamps, Daytime Running Lamps
RR DFG | Green (30) | Rear Window Defogger (Feeds directly to REAR DEFOG)
TRS LP | Red (10) | Automatic Transaxle Line Pressure Solenoid
TRS 2/TCC | Red (10) | Automatic Transaxle 2nd Gear and Torque Converter Clutch Solenoid
TRS 3/4 | Red (10) | Automatic Transaxle 3rd Gear Solenoid and 4th Gear Solenoid
MISCELLANEOUS DEVICES
A/C Diode |  | AC Diode (for Electrical System Protection)
OIL-R |  | Oil Life Reset Button

The following chart lists the relays, located in the underhood fuse block, and the system they control.

Note: A label is provided on the fuse block cover for relay layout.

#### Underhood Fuse Block Relays

RELAY | SYSTEM
--- | ---
A/C | Air Conditioning
AIR PUMP | Air Pump
COOL FAN | Engine Cooling
DRL | Daytime Running Lamps
FOG LAMP | Fog Lamps
HORN | Horn

The following chart lists the minifuses, located in the instrument fuse block, and the system they control.

Note: A label is provided on the fuse block cover for fuse layout.

#### Instrument Panel Fuse Block Minifuses

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
AIR BAG | Red (10) | Air Bags, Sensing and Diagnostic Module (SDM)
BODY | Red (10) | Dome Lamp, Luggage Compartment Lamp, Power Mirrors, Map Lamps, Hatch Release (Wagon), Decklid Release (Sedan and Coupe), Power Door Locks , Body Control Module, Data Link Connector
BODY COMP | Red (10) | Body Control Module, Instrument Panel
CD (RIA) | Tan (5) | CD Changer/Player (Retailer Installed Accessory)
CRUISE 1 | Red (10) | Cruise Control Module, Stoplamp (Brake) Switch, Fresh Air Solenoid, Brake Transmission Shift Interlock, CRUISE2 (2 amp) Fuse
CRUISE 2 | Grey (2) | Cruise Control Switch
FUEL PUMP | Red (10) | Fuel Pump
HVAC | Blue (15) | Climate Control, Rear Defogger
IGN 1 | Red (10) | Instrument Panel Telltale Indicators & Gauges, Body Control Module
IGN 3 | Red (10) | Anti-Lock Brakes, Rear Defogger (Feeds directly to REAR DEFOG Relay)
LIGHTER | Yellow (20) | Cigar Lighter
LOCKS | Yellow (20) | Power Door Locks
RADIO (BAT) | Red (10) | Radio/Clock Memory
RADIO (IGN) | Red (10) | Radio, Body Control Module
SUN | Blue (15) | Power Sunroof, Rear Wiper/Washer (Wagon)
TURN | Red (10) | Turn Signals
WIPER | Natural (25) | Windshield Wipers and Washers (Front)

The following chart lists the relays and modules, located in the instrument panel fuse block, and the system they control.

Note: A label is provided on the fuse block access panel for relay layout.

#### Instrument Panel Fuse Block Relays/Modules

RELAY/MODULE | SYSTEM
--- | ---
FLASHER MODULE | Turn Signal/Hazard Flashers (Back Side of Instrument Panel Fuse Block)
FUEL PUMP Relay | Fuel Pump, Transaxle Solenoids
HVAC BLOWER Relay | HVAC Blower Motor
LOCK Relay | Door Lock
REAR DEFOG Relay | Rear Defogger
UNLOCK Relay | Door Unlock
WINDOW Relay | Power Windows, Power Sunroof, Rear Wiper/Washer (Wagon)