For 1990-2009 cars

Table 1: | Body to Engine Inline
Table 2: | Body Harness to Headliner Inline-Sedan
Table 3: | Body Harness to Headliner Inline-Wagon, Coupe
Table 4: | Body to I/P Inline Body Side Connector-Sedan, Coupe
Table 5: | Body to I/P Inline Body Side Connector-Wagon
Table 6: | Body to I/P Inline I/P Side Connector
Table 7: | CD Jumper Inline (F)-Body Harness
Table 8: | CD Jumper Inline (M)-Jumper Harness
Table 9: | Decklid Inline-to Decklid Harness-Sedan
Table 10: | Decklid Inline-to Decklid harness-Coupe
Table 11: | Decklid Inline-to Body Harness-Coupe
Table 12: | Decklid Inline-to Body Harness-Sedan
Table 13: | Engine to Body-Inline
Table 14: | Fuel Tank Inline-M
Table 15: | Fuel Tank Inline-M
Table 16: | Headliner Inline to Body Harness-Sedan
Table 17: | Headliner Inline to Body Harness-Wagon, Coupe
Table 18: | License LampsHarness Inline-Decklid Harness-Coupe Only
Table 19: | Liftgate Inline-Wagon-Body Harness
Table 20: | Liftgate Inline-Wagon-Liftgate Harness
Table 21: | Liftgate Inline-Wagon-Body Harness
Table 22: | Liftgate Inline-Wagon-Liftgate Harness
Table 23: | Liftgate Inline-Wagon-Body Harness
Table 24: | Liftgate Inline-Wagon-Body Harness
Table 25: | Radio W/O CD Changer Jumper or CD Jumper Inline Harness W/ CD Changer Jumper
Table 26: | Stop/Tail/Back-up/Turn/Marker Lamp Inline-Right
Table 27: | Stop/Tail/Back-up/Turn/Marker Lamp Inline-Left
Table 28: | Sunroof to Body Inline-Sunroof Side Connector
Table 29: | Sunroof to Body Inline Body Side Connector-Sedan/Coupe

#### Body to Engine Inline

Connector Part Information |

• | 12047886

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | CircuitFunction
--- | --- | --- | --- | ---
A | WHT | 1310B | .35 | EVAP CANISTER VENT VALVE OUT
B | DK GRN | 890B | .35 | FUEL TANK PRESSURE SENSOR IN
C | -- | -- | -- | --
D | PPL | 30A | .35 | FUEL LEVEL IN
E | BLK/WHT | 251B | .35 | FUEL LEVEL RETURN
F | -- | -- | -- | --
G | -- | -- | -- | --
H | ORN/BLK | 469B | .35 | FUEL TANK PRESSURE SENSOR RETURN
Location: Hinge Pillar -- Left Front

#### Body Harness to Headliner Inline-Sedan

Connector Part Information |

• | 12103377

• | ENTER PART DESCRIPTION HERE

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 156A 156B | .35 | DOME SWITCH-W/O RKE DOME SWITCH-W/ RKE
B | BLK | 550T | .35 | DOME GROUND
C | ORN | 340A | .35 | DOME BULB
Location: Left B-Pillar

#### Body Harness to Headliner Inline-Wagon, Coupe

Connector Part Information |

• | 12084256

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 156A 156B | .35 |
B | BLK ORN | 550T 340A | .35 | DOME SWITCH W/O RKE DOME SWITCH W/ RKE
C | ORN BLK | 340A 550T | .35 | DOME GROUND-SW B+ TO DOME BULB --SC
D | ORN/BLK LT BLU | 737 20B | .35 | DOME BULB --SW DOME GROUND-SC
E | BLK | 550AT 550V | .35 | CARGO LP GROUND --SW CHMSL GROUND --SC
F | ORN | 440A | .35 | CARGO LP BULB -- SW
Location: Left D-Pillar-Upper Rear --Wagon Left B-Pillar-Coupe

#### Body to I/P Inline Body Side Connector-Sedan, Coupe

Connector Part Information |

• | 12092248

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | -- | -- | -- | --
B | -- | -- | -- | --
C | LT GRN | 200 200B | .35 | RT FRT SPKR+
D | DK GRN | 117 117B | .35 | RT FRT SPKR-
E | TAN | 201 201C | .35 | LT FRT SPKR+
F | GRA | 118 118C | .35 | LT FRT SPKR-
G | LT BLU | 20B 20K | .50 | BRAKES-CHMSL-SC BRAKES-CHMSL-SL
H | BLK | 28C | .35 | RKE HORN FUNCTION
J | LT BLU | 1344B | .35 | RKE DECKLID FUNCTION
K | LT BLU | 20C 20E | .50 | BRAKES-STOP LAMPS
L | -- | -- | -- | --
M | LT GRN | 24G,H 24E,F | .35 | BACK-UP LAMPS-SC BACK-UP LAMPS-SL
N | BLK | 884CR | .80 | LT REAR WHEEL SENSOR
P | RED | 885CR | .80 | LT REAR WHEEL SENSOR
R | WHT | 883CP | .80 | RT REAR WHEEL SENSOR
S | BRN | 882CP | .80 | RT REAR WHEEL SENSOR
T | YEL/BLK | 625A | .35 | CRANK ENABLE
U | GRA | 416J | .35 | 5 V REF FUEL PRESSURE SENSOR
V | BRN | 199 | .35 | LT REAR SPKR+
W | YEL | 116 | .35 | LT REAR SPKR-
X | DK BLU | 46 | .35 | RT REAR SPKR+
Y | LT BLU | 115 | .35 | RT REAR SPKR-
Z | BLK/WHT | 1455A | .35 | RKE PROGRAM FUNCTION
Location: Hinge Pillar-Left Front

#### Body to I/P Inline Body Side Connector-Wagon

Connector Part Information |

• | 12092248

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN | 392B | .50 | REAR WINDOW WASHER PUMP MOTOR-HIGH
B | WHT | 393B | .50 | REAR WINDOW WIPER PUMP MOTOR-HIGH
C | LT GRN | 200 200B | .35 | RT FRT SPKR+
D | DK GRN | 117 117B | .35 | RT FRT SPKR-
E | TAN | 201 201C | .35 | LT FRT SPKR+
F | GRA | 118 118C | .35 | LT FRT SPKR-
G | LT BLU | 20N | .50 | BRAKES CHMSL
H | BLK | 28C | .35 | RKE HORN FUNCTION
J | LT BLU | 1344B | .35 | RKE LIFTGATE FUNCTION
K | LT BLU | 20L 20M | .50 | BRAKES-STOP LAMPS
L | DK GRN | 146 | .35 | CARGO LAMP SWITCH
M | LT GRN | 24L 24M | .35 | BACK-UP LAMPS
N | BLK | 884CR | .80 | LT REAR WHEEL SENSOR
P | RED | 885CR | .80 | LT REAR WHEEL SENSOR
R | WHT | 883CP | .80 | RT REAR WHEEL SENSOR
S | BRN | 882CP | .80 | RT REAR WHEEL SENSOR
T | YEL/BLK | 625A | .35 | CRANK ENABLE
U | GRA | 416J | .35 | 5 V REF FUEL PRESSURE SENSOR
V | BRN | 199 | .35 | LT REAR SPKR+
W | YEL | 116 | .35 | LT REAR SPKR-
X | DK BLU | 46 | .35 | RT REAR SPKR+
Y | LT BLU | 115 | .35 | RT REAR SPKR-
Z | BLK/WHT | 1455A | .35 | RKE PROGRAM FUNCTION
Location: Hinge Pillar-Left Front

#### Body to I/P Inline I/P Side Connector

Connector Part Information |

• | 12092249

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN | 392A | .50 | REAR WIPER PUMP SWITCH-SW
B | WHT | 393A | .50 | REAR WIPER SWITCH-SW
C | LT GRN | 200A | .35 | RT FRT SPKR+
D | DK GRN | 117A | .35 | RT FRT SPKR-
E | TAN | 201A | .35 | LT FRT SPKR+
F | GRA | 118A | .35 | LT FRT SPKR-
G | LT BLU | 20H | .50 | BRAKE SWITCH
H | BLK | 28B | .35 | RKE HORN FUNCTION
J | LT BLU | 1344A | .35 | RKE DECKLID/LIFTGATE FUNCTION
K | LT BLU | 20F | .50 | BRAKE SWITCH
L | DK GRN | 146A | .35 | TAILGATE TT-SW
M | LT GRN | 24A | 2.0 | BACK-UP LAMP SWITCH
N | BLK | 884CF | .35 | ABS CONTROLLER
P | RED | 885CF | .35 | ABS CONTROLLER
R | WHT | 883CG | .35 | ABS CONTROLLER
S | BRN | 882CG | .35 | ABS CONTROLLER
T | YEL/BLK | 625 | .35 | CRANK ENABLE
U | GRA | 416H | .35 | 5 V REF FUEL PRESSURE SENSOR
V | BN | 199A | .35 | LT REAR SPKR+
W | YEL | 116A | .35 | LT REAR SPKR-
X | DK BLU | 46A | .35 | RT REAR SPKR+
Y | LT BLU | 115A | .35 | RT REAR SPKR-
Z | BLK/WHT | 1455B | .35 | RKE PROGRAM FUNCTION
Location: Hinge Pillar-Left Front

#### CD Jumper Inline (F)-Body Harness

Connector Part Information |

• | 12064769

• | Natural

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN/WHT | 367 | .35 | LEFT AUDIO
B | BLK/WHT | 372 | .35 | AUDIO COMMON
C | DK GRN/WHT | 368 | .35 | RIGHT AUDIO
D | BARE | 514 | .35 | GROUND-SHIELD
E | DK GRN | 835 | .35 | E/C DATA LINE
F | BKL | 350 | 1.0 | GROUND
G | ORN | 440 | .35 | POWER
Location: I/P Center-Under Front of Console

#### CD Jumper Inline (M)-Jumper Harness

Connector Part Information |

• | 12064770

• | Natural

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN/WHT | 367A | .35 | LEFT AUDIO
B | BLK/WHT | 372A | .35 | AUDIO COMMON
C | DK GRN/WHT | 368A | .35 | RIGHT AUDIO
D | BARE | 514A | .35 | GROUND-SHIELD
E | DK GRN | 835A | .35 | E/C DATA LINE
F | BKL | 350A | 1.0 | GROUND
G | ORN | 440A | .35 | POWER
Location: I/P Center-Under Front of Console

#### Decklid Inline-to Decklid Harness-Sedan

Connector Part Information |

• | 12077777

• | Blue

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 9R | .35 | TO LICENSE-L
B | BLK | 550CC | .50 | LICENSE LR GROUND-L
C | BRN | 9H | .35 | TO LICENSE LP-R
D | BLK | 550W | .50 | LICENSE LP GROUND-R
E | BLK | 550DE | .35 | GROUND TERMINAL
F | RED/BLK | 744 | .35 | TO CARGO LP SW
G | GRA | 382A | .35 | TO DECKLID RELEASE MOTOR
H | BLK | 550AA | .35 | DECKLID RELEASE MOTOR GROUND
lOCATION: rEAR cOMPARTMENT-lEFT rEAR sHOCK tOWER

#### Decklid Inline-to Decklid harness-Coupe

Connector Part Information |

• | 12078169

• | Natural

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT GRN | 24G | .35 | TO RIGHT BACKUP LAMP
B | BLK | 550XX | .35 | RIGHT BACKUP LAMP GROUND
C | BRN | 9P | .35 | TO LICENSE LAMPS
D | BLK | 550VV | .35 | LICENSE LAMPS GROUND
E | LT GRN | 24H | .35 | TO LEFT BACKUP LAMP
F | BLK | 550WW | .35 | LEFT BACKUP LAMP GROUND
G | BLK | 550DZ | .35 | CARGO LAMP GROUND
H | RED/BLK | 744BB | .35 | CARGO LAMP CONTROL
J | BLK | 550LL | .35 | DECKLID RELEASE MOTOR GROUND
K | GRA | 382AA | .35 | DECKLID RELEASE MOTOR FEED
Location: Rear Compartment-Left Rear Shock Tower

#### Decklid Inline-to Body Harness-Coupe

Connector Part Information |

• | 12064769

• | Natural

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT GRN | 24J | .80 | TO RIGHT BACKUP LAMP
B | BLK | 550AE | .80 | RIGHT BACKUP LAMP GROUND
C | BRN | 9AR | .50 | TO LICENSE LAMP
D | BLK | 550AU | .50 | LICENSE LAMPS GROUND
E | LT GRN | 24K | .80 | TO LEFT BACKUP LAMP
F | BLK | 550AW | .80 | LEFT BACKUP LAMP GROUND
G | BLK | 550BY | .80 | CARGO LAMP GROUND
H | RED/BLK | 744C | .35 | CARGO LAMP CONTROL
J | BLK | 550RL | .35 | DECKLID RELEASE MOTOR GROUND
K | GRA | 382C | .35 | DECKLID RELEASE MOTOR FEED
Location: Rear Compartment -- Left Rear Shock Tower

#### Decklid Inline-to Body Harness-Sedan

Connector Part Information |

• | 12064766

• | Blue

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 9W | .50 | TO LICENSE LP--L
B | BLK | 550AB | .50 | LICENSE LR GROUND--L
C | BRN | 9X | .50 | TO LICENSE LP--R
D | BLK | 550AC | .50 | LICENSE LP GROUND--R
E | BLK | 550ZQ | 1.0 | GROUND TERMINAL
F | RED/BLK | 744A | .35 | TO CARGO LP SW
G | GRA | 382B | .35 | TO DECKLID ELEASE MOTOR
H | BLK | 550RA | .35 | DECKLID RELEASE MOTOR GROUND
Location: Rear Compartment -- Left Rear Shock Tower

#### Engine to Body-Inline

Connector Part Information |

• | 12084256

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 1310A | .35 | EVAP CANISTER VENT VALVE OUT
B | DK GRN | 890A | .35 | FUEL PRESSURE SENSOR IN
C | -- | -- | -- | --
D | PPL | 30E, EM | .35 | FUEL LEVEL IN
E | BLK/WHT | 251E | .35 | FUKEL LEVEL RETURN
F | -- | -- | -- | --
G | -- | -- | -- | --
H | ORN/BLK | 469B | .35 | FUEL TANK PRESSURE SENSOR RETURN
Location: Hinge Pillar-Left Front

#### Fuel Tank Inline-M

Connector Part Information |

• | 12020397

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | GRA | 120A | .80 | FUEL PUMP FEED
B | PPL | 30B | .80 | FUEL LEVEL SENSOR
C | BLK/WHT | 251E | .80 | FUEL LEVEL SENSOR
Location: Rear Compartment -- Left

#### Fuel Tank Inline-M

Connector Part Information |

• | 12020398

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | GRA | 120 | 1.0 | FUEL PUMP FEED
B | PPL | 30A | .35 | FUEL LEVEL SENSOR
C | BLK/WHT | 251B | .35 | FUEL LEVEL SENSOR
Location: Rear Compartment -- Left

#### Headliner Inline to Body Harness-Sedan

Connector Part Information |

• | 12047781

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 156B | .35 | DOME SWITCH
B | BLK | 550T | .35 | DOME GROUND
C | ORN | 340A | .35 | B+ TO DOME BULB
Location: Left B-Pillar

#### Headliner Inline to Body Harness-Wagon, Coupe

Connector Part Information |

• | 12047786

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 156B | .35-SW .80-SC | DOME SWITCH
B | BLK ORN | 550 340 | .35 .80 | DOME GROUND-SW B+ TO DOME BULB-SC
C | ORN BLK | 340 550A | .35 .80 | B+ TO DOME BULB-SW DOME GROUND-SC
D | ORN/BLK LT BLI | 737 20B | .35 .80 | CARGO LP SWITCH-SW TO CHMSL-SC
E | BLK | 550AT 550V | .35 .80 | CARGO LP GROUND-SW CHMSL GROUND-SC
F | ORN | 440A | .35 | CARGO LP BULB-SW
Location: Left D-Pillar-Upper Rear-Wagon Left B-Pillar-Coupe

#### License LampsHarness Inline-Decklid Harness-Coupe Only

Connector Part Information |

• | 12052641

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 9AR | .50 | POWER
B | BLK | 550AU | .50 | GROUND
Location: Rear of Decklid

#### Liftgate Inline-Wagon-Body Harness

Connector Part Information |

• | 12064766

• | Blue

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 9 | .35 | PARK/TAIL LAMPS
B | PNK | 580A | .50 | REAR WIPER MOTOR
C | WHT | 393B | .50 | REAR WIPER MOTOR
D | LT BLU | 20N | .50 | STOP LAMPS
E | BLK | 550AG | .50 | GROUND
F | BLK | 550AM | .50 | GROUND
G | GRA | 382B 382G | .35 | LIFTGATE RELEASE-W/ RKE LIFTGATE RELEASE-W/O RKE
H | BLK | 550AY | .35 | GROUND-CARGO LAMP/AJAR TT
Location: Roof-Rear Center

#### Liftgate Inline-Wagon-Liftgate Harness

Connector Part Information |

• | 12064767

• | Blue

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 9U | .50 | PARK/TAIL LAMPS
B | ORN | 580F | .50 | REAR WIPER MOTOR
C | WHT | 393C | .50 | REAR WIPER MOTOR
D | LT BLU | 20J | .50 | STOP LAMPS
E | BLK | 550EB | .50 | GROUND
F | BLK | 550EA | .35 | GROUND
G | GRA | 382F | .35 | TO LIFTGATE RELEASE
H | BLK | 550AX | .35 | GROUND
Location: Roof-Rear Center

#### Liftgate Inline-Wagon-Body Harness

Connector Part Information |

• | 12129136

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 293 | 2.0 | RT REAR DEFOG +
B | BLK | 550AK | 2.0 | LT REAR DEFOG --
C | ORN/BLK DK GRN | 737 146 | .35 | TO CARGO LAMP BULB CARGO LAMP SW +
D | BLK | 550EG | .35 | GROUND
Location: Roof-Rear Center

#### Liftgate Inline-Wagon-Liftgate Harness

Connector Part Information |

• | 12129135

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 293A | 2.0 | REAR DEFOG +
B | BLK | 550EC | 2.0 | REAR DEFOG GROUND
C | DK GRN | 146B | .35 | CARGO LAMP SW +
D | BLK | 550EH | .35 | GROUND
Location: Roof-Rear Center

#### Liftgate Inline-Wagon-Body Harness

Connector Part Information |

• | 12064760

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT BLU | 115 | .35 | RR SPEAKER --
B | DK BLU | 46 | .35 | RR SPEAKER +
C | BRN | 199 | .35 | LR SPEAKER +
D | YEL | 116 | .35 | LR SPEAKER --
Location: Roof-Rear Center

#### Liftgate Inline-Wagon-Body Harness

Connector Part Information |

• | 12064761

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT BLU | 115B | .35 | RR SPEAKER --
B | DK BLU | 46B | .35 | RR SPEAKER +
C | BRN | 199C | .35 | LR SPEAKER +
D | YEL | 116C | .35 | LR SPEAKER --
Location: Roof-Rear Center

#### Radio W/O CD Changer Jumper or CD Jumper Inline Harness W/ CD Changer Jumper

Connector Part Information |

• | 12092900

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | GRA | 118A | .35 | LF SPEAKER -
2 | TAN | 201A | .35 | LF SPEAKER +
3 | DK GRN | 117A | .35 | RF SPEAKER -
4 | LT GRN | 200A | .35 | FR SPEAKER +
5 | BLK | 350A | 1.0 | GROUND
6 | BRN | 9M | .35 | PARK LAMPS ON
7 | DK GRN | 44H | .35 | DIMMER ILLUM
8 | -- | -- | -- | --
9 | YEL | 43 | .35 | IGN 4
10 | ORN | 440F | .35 | BATT+
17 | LT BLU | 115A | .35 | RR SPEAKER -
18 | DK BLU | 46A | .35 | RR SPEAKER+
19 | YEL | 116A | .35 | LR SPEAKER -
20 | BRN | 199A | .35 | LR SPEAKER +
Location:I/P Center-Behind Radio

#### Stop/Tail/Back-up/Turn/Marker Lamp Inline-Right

Connector Part Information |

• | 12052848

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN | 19 | .80 | TURN LAMPS
B | BRN | 9G-SL, SC 9Z-SW | .35 | TAIL LAMPS
C | BLK | 550Y-SL 550AJ-SW 550PP-SC | 1.0 | GROUND
D | LT BLU | 20E-SL, SC 20L-SW | .50 | STOP LAMPS
E | -- | -- | -- | --
F | LT GRN | *24E-SL 24H-SW | .35 | BACK-UP LAMP
Location: Rear Compartment-Right * 1st Design

#### Stop/Tail/Back-up/Turn/Marker Lamp Inline-Left

Connector Part Information |

• | 12052848

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 18 | 1.0 | TURN LAMP
B | BRN | 9F-SL, SC 9Y-SW | .35 | TAIL LAMPS
C | BLK | 550X-SL 550AR-SW 550NN-SC | 1.0 | GROUND
D | LT BLU | 20C-SL, SC 20N-SW | .50 | STOP LAMPS
E | -- | -- | -- | --
F | LT GRN | *24F-SL 24L-SW | .35 | BACK-UP LAMP
Location: Rear Compartment-Left * 1st Design

#### Sunroof to Body Inline-Sunroof Side Connector

Connector Part Information |

• | 12064760

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 550FF | .35 | MAP LIGHT GROUND
B | ORN | 340G | .35 | MAP LIGHT POWER
C | ORN | 580C | .50 | SUNROOF POWER
D | BLK | 550GG | .50 | SUNROOF GROUND
Location: Right B-Pillar Base

#### Sunroof to Body Inline Body Side Connector-Sedan/Coupe

Connector Part Information |

• | 12065658

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 550BB | .35 | MAPLIGHT GROUND
B | ORN/BLK | 340F | .35 | MAPLIGHT POWER
C | ORN | 580-SL 580B-SC | .50 | SUNROOF POWER
D | BLK | 550N | .50 | SUNROOFGROUND
Location: Right B-Pillar Base