For 1990-2009 cars

Table 1: | Cooling Fan Motor
Table 2: | Coolant Level Switch
Table 3: | Engine Coolant Temperature Sensor
Table 4: | Vehicle Speed Sensor (VSS)

#### Cooling Fan Motor

Connector Part Information |

• | 12103172

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 650 | 3.0 | GROUND
B | LT BLU | 409 | 3.0 | FROM COOLING FAN RELAY
Location: Engine Compartment-Center Front

#### Coolant Level Switch

Connector Part Information |

• | 12052641

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL/BLK | 68 | .35 | LOW COOLANT LEVEL OUTPUT
B | PNK | 239C | .35 | COOLANT LEVEL SW
Location: Coolant Bottle

#### Engine Coolant Temperature Sensor

Connector Part Information |

• | 12092512

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 410 | .35 | SENSOR INPUT SIGNAL
B | BLK | 452MA-Man 452M-Auto | .35 | RETURN
Location:Engine Compartment-Upper Left

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12052644

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 400-AUTO 400M-MAN | .35 | SIGNAL HI
B | PPL | 401-AUTO 401M-MAN | .35 | SIGNAL LO
Location: Engine Compartment-On Transaxle Diff