For 1990-2009 cars

#### Seat Belts Torque Specifications

Application | Specification
--- | ---
Metric | English
Child Safety Seat Tether Bracket Bolt | 20-30 N·m | 15-22 lb ft
Front Seat Shoulder Belt Guide Bracket Fasteners | 40 N·m | 30 lb ft
Presenter Arm Seat Belt Assembly -- Coupe | 50 N·m | 37 lb ft
Rear Seat Center Seat Belts Bolts | 50 N·m | 37 lb ft
Rear Shoulder Belt-to-Floor Bolt | 50 N·m | 37 lb ft
Seat Belt Bolt | 50 N·m | 37 lb ft
Seat Belt Rocker Fastener | 50 N·m | 37 lb ft
Seat Belt Slide Bar Fasteners | 50 N·m | 37 lb ft
Seat Belt Unit Retractor Fastener | 50 N·m | 37 lb ft
Seat Shoulder Belt Guide Fasteners | 5 N·m | 44 lb in
Seat Side Mount Buckle Bolts | 75 N·m | 55 lb ft
Shoulder Belt Lower Anchor Bolt | 50 N·m | 37 lb in