For 1990-2009 cars

Caution: Leaving children in a vehicle with the ignition key is dangerous for many reasons, children or others could be badly injured or even killed. They could operate the power windows or other controls or even make the vehicle move. The windows will function with the keys in the ignition and children could be seriously injured or killed if caught in the path of a closing window. Do not leave the keys in a vehicle with children.

The key furnished with your Saturn vehicle works the ignition and all locks.

An optional Valet key, that will operate your doors and ignition only , is available from your Saturn retailer. Refer to Valet Lockout Switch.

Key code information can be obtained at any Saturn retailer where your vehicle was purchased. These code numbers can be used to make new keys. Additional keys that are needed can be made at any Saturn retailer service facility provided you have the key code information. Store this information in a safe place, but NOT in your vehicle.

Notice: If you ever lock your keys in the vehicle, you may have to damage the vehicle to get in. Be sure you have spare keys.

### Lock Cylinder Lubrication

Lubricate the lock cylinders with a light oil or graphite lubricant. Never use a silicone spray lubricant, as these lubricants wash any existing oil from the lock cylinder and then evaporate, leaving less lubricant than before.