For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Seat Adjuster-to-Seat Bolts | 27 N·m | 20 lb ft
Front Seat Back Recliner Bolts | 27 N·m | 20 lb ft
Front Seat Cushion-to-Seat Adjuster | 27 N·m | 20 lb ft
Front Seat-to-Floor Panel Bolts | 30 N·m | 22 lb ft
Front Seatback Cushion Recliner Bolts | 27 N·m | 20 lb ft
Front Seatback Recliner Bolts | 27 N·m | 20 lb ft
Lumbar Actuator Fasteners | 3 N·m | 27 lb in
Rear Folding Seat Back Beam Fasteners | 18 N·m | 13 lb ft
Rear Folding Seat Back Latch Fasteners | 2 N·m | 18 lb in
Recliner Handle Fastener | 3 N·m | 27 lb in
Recliner Lever Fastener | 3 N·m | 27 lb in
Recliner-to-Seat Back | 27 N·m | 20 lb ft
Seat Belt Buckle-to-Seat Adjuster Bolt | 75 N·m | 55 lb ft
Seat Belt Guide-to-Headrest Fasteners | 5 N·m | 44 lb in
Seat Belt Shoulder Guide Fasteners | 5 N·m | 44 lb in