For 1990-2009 cars

Table 1: | CD Changer
Table 2: | Radio W/ CD Changer Jumper
Table 3: | Radio W/O CD Changer Jumper or CD Jumper Inline Harness W/ CD Changer Jumper
Table 4: | Speakers-Front/Rear
Table 5: | Speakers-Front/Rear-Right Front
Table 6: | Speakers-Front/Rear-Left Front
Table 7: | Speakers-Front/Rear-Right Rear
Table 8: | Speakers-Front/Rear-Left Rear

#### CD Changer

Connector Part Information |

• | 12047531

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | BRN/WHT | 367 | .35 | LEFT AUDIO OUT
2 | DK GRN/WHT | 368 | .35 | RIGHT AUDIO OUT
3 | BLK/WHT | 372 | .35 | AUDIO COMMON
4 | BARE | 514 | .35 | GROUND-SHIELD
5 | ORN | 440 | .35 | POWER
6 | -- | -- | -- | --
7 | BLK | 350 | 1.0 | GROUND
8 | -- | -- | -- | --
9 | -- | -- | -- | --
10 | DK GRN | 835 | .35 | E/C DATA LINE
Location: Rear Compartment-Under Package Shelf- back of CD Changer

#### Radio W/ CD Changer Jumper

Connector Part Information | Two Connectors LockedTtogether

• | 12047531

| 12065785

• | Black

| Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | GRA | 118 | .35 | LF SPEAKER -
2 | TAN | 201 | .35 | LF SPEAKER +
3 | DK GRN | 117 | .35 | RF SPEAKER -
4 | LT GRN | 200 | .35 | RF SPEAKER +
5 | BLK | 350A | 1.0 | GROUND
6 | BRN | 9 | .35 | PARK LAMPS ON
7 | DK GRN | 44 | .35 | DIMMER ILLUM
8 | -- | -- | -- | --
9 | YEL | 43 | .35 | IGN 4
10 | ORN | 440A | .35 | POWER
11 | BRN/WHT | 367 | .35 | LF AUDIO
12 | BLK/WHT | 372 | .35 | COMMON AUDIO
13 | DK GRN/WHT | 368 | .35 | RT AUDIO
14 | BARE | 514 | .35 | GROUND-SHIELD
15 | -- | -- | -- | --
16 | DK GRN | 835 | .35 | E/C DATA LINE
17 | LT BLU | 115 | .35 | RR SPEAKER -
18 | DK BLU | 46 | .35 | RR SPEAKER +
19 | YEL | 116 | .35 | LR SPEAKER -
20 | BRN | 199 | .35 | LR SPEAKER +
Location: I/P Center-Behind Radio

#### Radio W/O CD Changer Jumper or CD Jumper Inline Harness W/ CD Changer Jumper

Connector Part Information |

• | 12092900

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | GRA | 118A | .35 | LF SPEAKER -
2 | TAN | 201A | .35 | LF SPEAKER +
3 | DK GRN | 117A | .35 | RF SPEAKER -
4 | LT GRN | 200A | .35 | FR SPEAKER +
5 | BLK | 350A | 1.0 | GROUND
6 | BRN | 9M | .35 | PARK LAMPS ON
7 | DK GRN | 44H | .35 | DIMMER ILLUM
8 | -- | -- | -- | --
9 | YEL | 43 | .35 | IGN 4
10 | ORN | 440F | .35 | BATT+
17 | LT BLU | 115A | .35 | RR SPEAKER -
18 | DK BLU | 46A | .35 | RR SPEAKER+
19 | YEL | 116A | .35 | LR SPEAKER -
20 | BRN | 199A | .35 | LR SPEAKER +
Location:I/P Center-Behind Radio

#### Speakers-Front/Rear

Connector Part Information |

• | 12077887

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A |  |  |  |
B |  |  |  |

#### Speakers-Front/Rear-Right Front

Connector Part Information |

• | 12077887

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN | 117,117B | .35 | SPEAKER -
B | LT GRN | 200,200B | .35 | SPEAKER +
Location: Door-Front Right

#### Speakers-Front/Rear-Left Front

Connector Part Information |

• | 12077887

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | GRA | 118, 118C | .35 | SPEAKER _
B | TAN | 201, 201C | .35 | SPEAKER +
Location: Door Front Left

#### Speakers-Front/Rear-Right Rear

Connector Part Information |

• | 12077887

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT BLU | 115 | .35 | SPEAKER -
B | DK BLU | 46 | .35 | SPEAKER +
Location: Package Shelf- Right

#### Speakers-Front/Rear-Left Rear

Connector Part Information |

• | 12077887

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 116 | .35 | SPEAKER -
B | BRN | 119 | .35 | SPEAKER +
Location: Package Shelf-Left