For 1990-2009 cars

### Removal Procedure

1. Remove the bezel from the map lamp and the sunroof switch console by prying at the outside edge to unsnap the bezel.
2. Depress the tabs on the switch to remove and disconnect the wire connector from the switch.

### Installation Procedure

1. Connect the sunroof wire connector to the switch and push the switch into the roof console until the switch tabs engage.
2. Install the bezel into the map lamp and sunroof switch.