For 1990-2009 cars

DTC# | Description
--- | ---
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2
P0105 | MAP Sensor Circuit
P0107 | MAP Sensor Circuit Low Voltage
P0108 | MAP Sensor Circuit High Voltage
P0112 | IAT Sensor Circuit Low Voltage / High Temp.
P0113 | IAT Sensor Circuit High Voltage / Low Temp.
P0117 | ECT Sensor Circuit Low Voltage / High Temp.
P0118 | ECT Sensor Circuit High Voltage / Low Temp.
P0122 | TP Sensor Circuit Low Voltage
P0123 | TP Sensor Circuit High Voltage
P0125 | ECT Excessive Time to Closed Loop Fuel Control
P0130 | O2S Closed Loop Performance Sensor 1
P0131 | O2S Circuit Low Voltage Sensor 1
P0132 | O2S Circuit High Voltage Sensor 1
P0133 | O2S Slow Response Sensor 1
P0134 | O2S Circuit Insufficient Activity Sensor 1
P0137 | HO2S Circuit Low Voltage Sensor 2
P0138 | HO2S Circuit High Voltage Sensor 2
P0140 | HO2S Circuit Insufficient Activity Sensor 2
P0171 | Fuel Trim System Lean
P0172 | Fuel Trim System Rich
P0200 | Injector Control Circuit
P0217 | Engine Coolant Overtemperature
P0218 | Transmission Fluid Overtemperature
P0231 | Fuel Pump Relay Control Circuit Low Voltage
P0232 | Fuel Pump Relay Control Circuit High Voltage
P0261 | Injector 1 Control Circuit Low Voltage
P0262 | Injector 1 Control Circuit High Voltage
P0264 | Injector 2 Control Circuit Low Voltage
P0265 | Injector 2 Control Circuit High Voltage
P0267 | Injector 3 Control Circuit Low Voltage
P0268 | Injector 3 Control Circuit High Voltage
P0270 | Injector 4 Control Circuit Low Voltage
P0271 | Injector 4 Control Circuit High Voltage
P0300 | Engine Misfire Detected
P0324 | Knock Sensor Module Circuit
P0325 | Knock Sensor Module Circuit
P0326 | Knock Sensor System Performance
P0327 | Knock Sensor Circuit Low Frequency
P0336 | CKP Sensor Performance
P0340 | CMP Sensor Circuit
P0341 | CMP Sensor Performance
P0351 | Ignition Coil 1 and 4 Control Circuit
P0352 | Ignition Coil 2 and 3 Control Circuit
P0401 | EGR Flow Insufficient
P0403 | EGR Solenoid Control Circuit
P0404 | EGR Open Position Performance
P0405 | EGR Position Sensor Circuit Low Voltage
P0410 | AIR System
P0413 | AIR Solenoid Control Circuit Low Voltage
P0414 | AIR Solenoid Control Circuit High Voltage
P0418 | AIR Pump Relay Control Circuit Low Voltage
P0420 | Catalyst System Low Efficiency
P0440 | EVAP System
P0442 | EVAP System Small Leak Detected
P0444 | EVAP Purge Solenoid Control Circuit Low Voltage
P0445 | EVAP Purge Solenoid Control Circuit High Voltage
P0446 | EVAP Vent System Performance
P0447 | EVAP Vent Solenoid Control Circuit Low Voltage
P0448 | EVAP Vent Solenoid Control Circuit High Voltage
P0452 | Fuel Tank Pressure Sensor Circuit Low Voltage
P0453 | Fuel Tank Pressure Sensor Circuit High Voltage
P0461 | Fuel Level Sensor Performance
P0462 | Fuel Level Sensor Circuit Low Voltage
P0463 | Fuel Level Sensor Circuit High Voltage
P0480 | Cooling Fan Relay Control Circuit
P0500 | VSS Circuit
P0506 | Idle Speed Low
P0507 | Idle Speed High
P0508 | IAC Valve Control Circuit Low Voltage
P0509 | IAC Valve Control Circuit High Voltage
P0561 | System Voltage Performance
P0562 | System Voltage Low
P0563 | System Voltage High
P0565 | Cruise Control Switch Circuit
P0572 | Cruise Control Brake Switch Circuit Low Voltage
P0573 | Cruise Control Brake Switch Circuit High Voltage
P0601 | PCM Memory
P0602 | PCM Not Programmed
P0603 | PCM Long Term Memory Reset
P0606 | PCM Internal Performance
P0621 | Generator L - Terminal Circuit
P0636 | Steering Assist Solenoid Control Circuit Low Voltage
P0637 | Steering Assist Solenoid Control Circuit High Voltage
P0646 | A/C Clutch Relay Control Circuit Low Voltage
P0647 | A/C Clutch Relay Control Circuit High Voltage
P0702 | Transaxle Control System Low Voltage
P0705 | Transaxle Range Switch Circuit
P0706 | Transaxle Range Switch Performance
P0708 | Transaxle Range Switch Circuit High Voltage
P0710 | TFT Sensor Performance - Low Temp.
P0711 | TFT Sensor Performance
P0712 | TFT Sensor Circuit Low Voltage / High Temp.
P0713 | TFT Sensor Circuit High Voltage / Low Temp.
P0714 | TFT Sensor Circuit Intermittent
P0716 | ISS Sensor - Intermittent
P0717 | ISS Sensor - Low Input
P0721 | OSS Sensor Performance
P0722 | OSS Sensor Low Input
P0730 | No Gears Available
P0731 | Incorrect 1st Gear Ratio
P0732 | Incorrect 2nd Gear Ratio
P0733 | Incorrect 3rd Gear Ratio
P0734 | Incorrect 4th Gear Ratio
P0740 | TCC Solenoid Control Circuit Low Voltage
P0741 | TCC System Stuck Off
P0742 | TCC System Stuck On
P0743 | TCC Solenoid Control Circuit High Voltage
P0745 | PC Solenoid Pressure Low
P0746 | PC Solenoid Control Circuit Low Voltage
P0747 | PC Solenoid Control Circuit High Voltage
P0748 | Transmission Line Pressure High
P0756 | Shift Solenoid 2 Control Circuit Low Voltage
P0758 | Shift Solenoid 2 Control Circuit High Voltage
P0761 | Shift Solenoid 3 Control Circuit Low Voltage
P0763 | Shift Solenoid 3 Control Circuit High Voltage
P0766 | Shift Solenoid 4 Control Circuit Low Voltage
P0768 | Shift Solenoid 4 Control Circuit High Voltage
P0781 | Shift Solenoid 2 Performance
P0782 | Shift Solenoid 3 Performance
P0783 | Shift Solenoid 4 Performance
P0789 | Shift/Timing Solenoid Control Circuit Intermittent
P1133 | O2S Insufficient Switching Sensor 1
P1134 | O2S Transition Time Ratio Sensor 1
P1336 | CKP System Variation Not Learned
P1351 | Ignition Coil 1 and 4 Control Circuit High Voltage
P1352 | Ignition Coil 2 and 3 Control Circuit High Voltage
P1403 | EGR Solenoid Control Circuit Low Voltage
P1404 | EGR Closed Position Performance
P1418 | AIR Pump Relay Control Circuit High Voltage
P1441 | EVAP System Flow During Non-Purge
P1480 | Cooling Fan Relay Control Circuit High Voltage
P1580 | Cruise Control Move Output Circuit Low Voltage
P1581 | Cruise Control Move Output Circuit High Voltage
P1582 | Cruise Control Direction Output Circuit Low Voltage
P1583 | Cruise Control Direction Output Circuit High Voltage
P1584 | Cruise Control Disabled
P1587 | Cruise Control Clutch Output Circuit Low Voltage
P1588 | Cruise Control Clutch Output Circuit High Voltage
P1599 | Engine Stall or Near Stall Detected
P1620 | Low Engine Coolant Level
P1621 | PCM Long Term Memory Performance
P1624 | Customer Snapshot Requested Data Available
P1626 | Lost Class II Communications with BCM
P1630 | Theft Deterrent Learn Mode Active
P1631 | Theft Deterrent Fuel Enable Signal Not Correct
P1635 | 5 Volt Reference Circuit
P1816 | Transmission Range Switch - P/N w/Drive Ratio
B3538 | Oil Life Reset Switch Circuit Low
U1000 | Class II Data Link Malfunction
U1040 | Lost Communications with Brake/Traction Control System
U1064 | Lost Communications with Body Multiple Control System
U1096 | Lost Communications with Driver Information & Displays Control System
U1300 | Class II Data Link Low
U1301 | Class II Data Link High