For 1990-2009 cars

### (Option)

If you have this option, the switch is located above your rearview mirror.

When your ignition is in "RUN," press the "OPEN/VENT" portion of the switch to the first position to raise the rear of the sunroof to provide additional venting. Press the "OPEN/VENT" switch to the second position to fully open the roof.

To close the sunroof, press and hold the "CLOSE" portion of the switch.