For 1990-2009 cars

Table 1: | Liftgate Release Switch-Wagon
Table 2: | Liftgate Release Motor-Wagon
Table 3: | Remote Keyless Entry (RKE) Module

#### Liftgate Release Switch-Wagon

Connector Part Information |

• | 12052641

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | ORN | 340E | .35 | B+
B-w/ RKE | BLK | 1576 | .35 | RELEASE SWITCH OUTPUT
B W/O RKE | GRA | 832G | .35 | RELEASE SWITCH OUTPUT
Location: Liftgate Latch

#### Liftgate Release Motor-Wagon

Connector Part Information |

• | 12052641

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | GRA | 382F | .35 | SWITCHED B+
B | BLK | 550EH | .35 | GROUND
Location: On Liftgate Latch

#### Remote Keyless Entry (RKE) Module

Connector Part Information |

• | 12129431

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | TAN | 294K-SL, SW 294E-SC | .80 | DR DOOR UNLOCK OUTPUT
B | WHT | 194R | .35 | REMAINING DOORS UNLOCK OUTPUT
C | BLK | 28C | .35 | HORN CONTROL
D | YEL/BLK | 625A | .35 | STARTER RELAY CONTROL
E | ORN | 440R | .35 | POWER
F | -- | -- | -- | -
G | GRA | 382A-SL 382B-SW 382C-SC | .35 | DECKLID/LIFTGATE RELEASE OUTPUT
H | -- | -- | -- | --
J | PNK | 39R | .35 | IGN 1
K | WHT | 156C | .35 | DOOR JAMB, SWITCH INPUT
L | BLK/WHT | 1455A | .35 | PROGRAMMING ENABLE
M | LT BLU | 1344B | .35 | DECKLID/LIFTGATE RELEASE ENABLE
N | BLK | 550R | .35 | GROUND
P | -- | -- | -- | --
R | LT BLU | 195R | .35 | DOOR LOCK RELAY CONTROL
S | WHT | 156B | .35 | DOME LAMP CONTROL
Location: Right Rear Wheelwell-Under Right Side Lock Pillar Interior Trim