For 1990-2009 cars

Table 1: | POD Switches-Fog Lamp/Traction/Rear Defog Switch
Table 2: | Rear Window Defog-Right
Table 3: | Rear Window Defog-Left

#### POD Switches-Fog Lamp/Traction/Rear Defog Switch

Connector Part Information |

• | 121295622

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | YEL | 317 | .35 | FOG LAMP RELAY CONTROL
B | PNK | 1200 | .35 | HI BEAM INPUT
C | PPL/WHT | 1572 | .35 | TRACTION CONT ENABLE
D | LT BLU | 292 | .35 | REAR DEFOG SW ON/OFF
E-G | -- | -- | -- | --
H | BLK | 350J | .35 | POD SWITCHES GROUND
J | WHT | 193 | .35 | REAR DEFOG RELAY/ON LED CONTROL
K | BRN | 641E | .35 | TRACTION CONT/REAR DEFOG ING3 FEED
L | DK GRN | 44L | .35 | POD SWITCHES ILLUMINATION
M | BRN | 9AN | .35 | POD SWITCHES ILLUMINATION
Location: I/P Center

#### Rear Window Defog-Right

Connector Part Information |

• | 12092582

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK BLK | 550HH-sc 550JJ-sl 293A | 2.0 2.0 2.0 | REAR DEFOG-LOW-SL/SC REAR DEFOG-LOW-SL REAR DEFOG-HIGH-SW
Location: Right Back Window

#### Rear Window Defog-Left

Connector Part Information |

• | 12092582

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 293 550EC | 2.0 2.0 | REAR DEFOG-HIGH-SL/SC REAR DEFOG-LOW-SW
Location: Left Back Window