For 1990-2009 cars

Complaint/Condition | Possible Causes | Corrections
--- | --- | ---
Vehicle pulls | Mismatched, unevenly worn, or improperly inflated tires | Replace or inflate tires correctly.
Improper front or rear wheel alignment | Correct wheel alignment.
Worn or bent front or rear suspension components | Replace components.
Worn wheel bearings | Replace wheel bearings.
Steering gear out of adjustment or worn | Replace or adjust steering gear.
Damaged or sagging springs | Replace springs.
Abnormal or excessive tire wear | Improper front or rear wheel alignment | Correct wheel alignment.
Worn struts | Replace struts.
Worn or bent front or rear suspension components | Replace components.
Hard driving | Advise customer.
Tires improperly inflated | Inflate tires correctly.
Excessive body roll/pitching | Worn struts | Replace worn struts.
Front stabilizer shaft bent or broken | Replace front stabilizer shaft.
Rear stabilizer shaft or stabilizer shaft links bent or broken | Replace rear stabilizer shaft/stabilizer shaft links.
Broken or sagging springs | Replace damaged springs.
Tires improperly inflated | Inflate tires correctly.