For 1990-2009 cars

# RATTLE NOISE IN 2ND GEAR DURING LEFT HAND TURNS

#### SUBJECT: Rattle Noise in 2nd Gear During Left Hand Turns - MP2/MP3 Manual Transaxles (Replace Reverse Shift Lever)

#### MODELS AFFECTED: 1991-1996 Saturns equipped with MP2/MP3 manual transaxles

CONDITION: Some customers may comment about a rattle noise when turning left while in 2nd gear.

CAUSE: The rattle noise may be caused by a damaged reverse shift lever assembly or a broken reverse shift lever spring that allows the reverse idler gear assembly to make contact with the 1st/2nd & Reverse synchronizer when the vehicle is turning left while in 2nd gear.

CORRECTION: Replace the damaged reverse shift lever assembly. Also, inspect the reverse idler gear assembly and 1st/2nd & Reverse synchronizer for damage or excessive wear, and replace if necessary. (Refer to appropriate year "Manual Transaxle" service manual for repair procedures.)

PARTS REQUIREMENTS: 21120283 Lever Asm - Rev Shift

CLAIM INFORMATION: To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System using the appropriate Electronic Labor Time Guide for the correct Labor Operation Code and Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.