For 1990-2009 cars

## Windshield Washer Fluid All Models

### What to Use

When you need windshield washer fluid (Saturn P/N 01051515), be sure to read the instructions before use. If you will be operating your vehicle in an area where the temperature may fall below freezing, use a fluid that has sufficient protection against freezing.

### Adding Windshield Washer Fluid

Open the cap labeled "WASHER FLUID" and add washer fluid until the tank is full.

Notice:

• | When using concentrated washer fluid, follow the manufacturer's instructions for adding water.

• | Do not mix water with ready-to-use washer fluid. Water can cause the solution to freeze and damage your washer fluid tank and other parts of the washer system. Also, water does not clean as well as washer fluid.

• | Fill the washer fluid tank only three-quarters full when it is very cold. This allows for fluid expansion if freezing occurs, which could damage the tank if it is completely full.

• | Do not use engine coolant (antifreeze) in your windshield washer. It can damage the vehicle's windshield washer system and paint.

## Windshield Washer Fluid Wagon Model Only

The rear window washer reservoir is located behind the interior trim panel on the right side of the rear cargo area.

To fill the reservoir, remove the plastic access cover by pulling at the finger tab. Once the access cover is removed, swing the reservoir filler neck out and remove the cap. Fill the reservoir with washer fluid to the top of the bottle at the base of the neck.