For 1990-2009 cars

Application | Specifications
--- | ---
Torque Spec Description | Metric | English
Control Arm-to-Frame Bolt | 125 | 92 lb ft
Control Arm-to-Frame-Nut | 100 | 74 lb ft
Control Arm-to-Front Stabilizer Shaft Nut | 144 | 106 lb ft
Crossmember-to-Body Fastener | 120 | 89 lb ft
Front Stabilizer Shaft Attachment Bracket-to-Frame | 140 | 103 lb ft
Front Stabilizer Shaft-to-Frame Nut | 140 | 103 lb ft
Front Strut Assembly-to-Body Attachment Nuts | 29 | 21 lb ft
Front Strut-to-Steering Knuckle Fasteners | 170 | 126 lb ft
Lateral Link-to-Crossmember Fastener | 120 | 89 lb ft
Lateral Link-to-Knuckle Fastener | 165 | 122 lb ft
Rear Stabilizer Shaft Link-to-Bracket | 40 | 30 lb ft
Rear Stabilizer Shaft-to-Crossmember | 55 | 41 lb ft
Rear Stabilizer Shaft-to-Link Fastener | 40 | 30 lb ft
Rear Strut Assembly-to-Body Attachment Nut | 29 | 21 lb ft
Rear Strut Shaft Nut | 50 | 37 lb ft
Rear Strut-to-Knuckle Fasteners | 170 | 126 lb ft
Rear Strut-to-Steering Knuckle Fasteners | 170 | 126 lb ft
Rear Wheel Hub Assembly | 85 | 63 lb ft
Trailing Arm-to-Body Fasteners | 120 | 89 lb ft
Trailing Arm-to-Knuckle Fasteners | 100 | 74 lb ft
Upper Strut Shaft Nut | 50 | 37 lb ft
Wheel Nuts | 140 | 103 lb ft