For 1990-2009 cars

#### Circuit Charts

SYMPTOM | PROCEDURE
--- | ---
All of the windows are inoperative from all of the switches. | Chart 1
Only the left front or only the right front window is inoperable. | Chart 2
The left rear or right rear window is inoperable from both the power window/mirror switch in the console and from the rear door window switch (Sedan and Wagon only). | Chart 3
The left rear or right rear window is inoperable from its rear door window switch only (Sedan and Wagon only). | Chart 4
The left rear or right rear window is inoperable from only the power window/mirror switch in the console. | Chart 5
Both the left rear and right rear windows are inoperable from the rear door window switches. |

• | Verify that the rear window lockout switch is in the ON position.

• | If the rear doors will not function when the rear window lockout switch is in the ON position, replace the power window/mirror switch in the console.

• | Check the power window operation from all window switches.

Rear window lockout switch does not lockout the rear door window switches. |

• | Verify that the rear window lockout switch is in the OFF position.

• | If the rear doors still function in the OFF position, replace the Power Window/Mirror Switch in the console.

• | Check power window operation from all window switches.

The front window auto down is inoperable. |

• | Verify that the auto down feature is inoperable.

• | Replace the power window/mirror switch in the console.

• | Check the motor and replace if necessary.

• | Check for mechanical/binding problems and fix if necessary.

• | Check the power window operation from all window switches.

A window will not go down all the way. |

• | Check for mechanical/binding problem and fix if necessary.

• | Check the ground (BLK circuit 550) between the power window/mirror switch terminal A and a known good ground.

• | Checkthe motor and replace if necessary.

• | Check the power window operation from all window switches.

### Chart 1

### Chart 2

### Chart 3

### Chart 4

### Chart 5