For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Stud Castle Nut

- First Pass

10 N·m

89 lb in

- Final Pass

+ 180°

Frame to Body Bolts | 155 N·m | 114 lb ft
Frame Reinforcement-to-Body Bolts (L66 only) | 50 N·m | 37 lb ft
Front Transaxle Mount Through Bolt | 110 N·m | 81 lb ft
Rear Body Mount Bracket Bolts | 50 N·m | 37 lb ft
Rear Transaxle Mount to Frame Bolts | 50 N·m | 37 lb ft
Stabilizer Shaft Clamp Bolt | 50 N·m | 37 lb ft
Steering Gear to Frame Bolts | 110 N·m | 81 lb ft