For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Antenna Bracket-to-Fender Fasteners | 10 N·m | 89 lb in
Antenna Mast-to-Antenna Base | 10 N·m | 89 lb in
CD Changer/Player-to-Console Fasteners - Front | 2.5 N·m | 22 lb in
CD Changer/Player-to-Console Fasteners - Rear | 4 N·m | 35 lb in
Console Front Fasteners | 2.2 N·m | 19 lb in
Console Rear Fasteners | 2.2 N·m | 19 lb in
Door Speaker Fasteners | 2.5 N·m | 22 lb in
I/P Endcap-to-I/P Fasteners | 2.2 N·m | 19 lb in
I/P Upper Trim Panel Fasteners | 6 N·m | 53 lb in
Liftgate Speaker Fasteners | 2.5 N·m | 22 lb in
Radio Ground Strap-to-H-Brace | 2.2 N·m | 19 lb in
Radio-to-I/P Fasteners | 2.5 N·m | 22 lb in
Steering Column Filler Panel Fasteners | 2.2 N·m | 19 lb in
Steering Column Shroud Fasteners | 1.5 N·m | 13 lb in