For 1990-2009 cars

The following table lists the security data directly connected to the body control module (BCM) related to the Passlock System only:

#### ABS/TCS Data Scan Tool Data List

Parameter | Unit
--- | ---
Battery 1 | Volts
Park Brake Switch | On/Off
Traction Switch | On/Off

#### Switch Inputs Scan Tool Data List

Parameter | Unit
--- | ---
A/C Request | Yes/No
Battery 1 | Volts
Driver Door Switch | Release/Applied
High Blower Input | Volts
HVAC Afterblow | On/Off
HVAC Afterblow Feedback | High/Low
Key In Ignition | Yes/No
Low Brake Fluid | Yes/No
Low Coolant | Yes/No
Park (BTSI) Relay Command | High/Low
Park (BTSI) Relay Feedback | High/Low
Park Brake Switch | On/Off
Passenger Door Switches | Release/Applied
Rear Defog Relay Command | On/Off
Rear Defog Relay Feedback | High/Low
Rear Defog Switch | On/Off

#### Exterior Lamps Scan Tool Data List

Parameter | Unit
--- | ---
Battery 1 | Volts
DRL Relay Command | On/Off
DRL Relay Feedback | High/Low
High Beam Input | Volts
Low Beam Input | Volts
Park Lamp Switch | On/Off

#### Interior Lamps Scan Tool Data List

Parameter | Unit
--- | ---
Battery 1 | Volts
Cargo Lamp On | On/Off
Dome Lamp Command | On/Off
Driver Door Switch | Release/Applied
I/P Dimmer Input | Volts
Inadvertent Load Monitor | On/Off
Key In Ignition | Yes/No
Passenger Door Switches | Release Applied

#### Door Locks Scan Tool Data List

Parameter | Unit
--- | ---
All Door Unlock Feedback | High/Low
All Door Unlock Relay Command | On/Off
Battery 1 | Volts
Driver Unlock Relay Command | On/Off
Driver Unlock Relay Feedback | High/Low
Lock All Relay Command | On/Off
Lock All Relay Feedback | High/Low
Passenger Unlock Relay Feedback | High/Low
Trunk Release Solenoid Command | On/Off
Trunk Release Solenoid Feedback | High/Low

#### Security Data Scan Tool Data List

Parameter | Unit
--- | ---
Accessory | High/Low
Auto-Learn Timer | Seconds
Battery 1 | Volts
Horn Relay Command | On/Off
Horn Relay Feedback | High/Low
Ignition 1 | High/Low
Lockout Timer | Seconds
Passenger lock Input | Volts
Passenger lock Power Command | On/Off
Passenger lock Power Feedback | High/Low
Security LED | On/Off/Flash
Seed and Key Timer | Seconds