INFORMATION ON FUEL TANK FILL CAP HOLDER RETAINER. Saturn Saturn 1994

For 1990-2009 cars

# INFORMATION ON FUEL TANK FILL CAP HOLDER RETAINER

#### SUBJECT: Fuel Tank Fill Cap Holder Retainer Installation to 1991-1995 Sedans/Wagons and 1991-1996 Coupes

#### MODELS AFFECTED: 1991-1995 Saturn Sedans, 1993-1995 Saturn Wagons and 1991-1996 Saturn Coupes

PURPOSE: This bulletin provides a procedure for installing the fuel tank fill cap holder retainer to the fuel fill door on the above mentioned vehicles, at customer's request.

#### PROCEDURE

1. Using a bench grinder, remove shaded areas of plastic from rearside of fuel tank fill cap holder retainer (P/N 21110502). This makes the rearside of the fuel tank fill cap holder retainer flush.

2. Clean surface of inner side of fuel door and rearside of fuel tank fill cap holder retainer with isopropyl alcohol to ensure adhesion of double sided foam tape to both surfaces.

3. Apply 3M SCOTCH-MOUNT Super Automotive Attachment Tape (P/N 06383) or equivalent double sided foam tape, to the rearside of the fuel tank fill cap holder retainer.

#### IMPORTANT: For best adhesion, vehicle surface should be at room temperature.

4. To determine vertical placement of fuel tank fill cap holder retainer on fuel door, measure 6 mm (1/4 in.) up from "Unleaded Fuel Only" decal placement marks on fuel door, and mark the location.

5. Remove backing paper from foam tape and position fuel tank fill cap holder retainer on fuel door with the bottom aligned with the mark made in step 4. The left edge of the fuel tank fill cap holder retainer will touch tab of fuel door as shown.

6. Press fuel tank fill cap holder retainer firmly in place on fuel door to ensure adhesion. Make sure not to exert too much pressure to prevent deforming fuel door.

PARTS REQUIREMENTS: 21110502 Retainer-Fuel Tank Fill Cap Holder

CLAIM INFORMATION: This repair should be handled as a customer pay transaction in the Saturn Dealer System. For Retailer purposes, the following can be used for billing purposes:

Labor Case Operation Type Description Code Time -------------------------------------------------------- CP Install Fuel Tank Fill Cap M5137 0.3 hrs Holder Retainer

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.