INFO. ON CONNECTOR POSITION ASSURANCE (CPA) RETAINER USAGE. Saturn Saturn 1991

For 1990-2009 cars

# INFO. ON CONNECTOR POSITION ASSURANCE (CPA) RETAINER USAGE

#### SUBJECT: SERVICE INFORMATION ON CONNECTOR POSITION ASSURANCE (CPA) RETAINER USAGE ON SATURN VEHICLES

#### MODELS AFFECTED: 1991-1994 SATURNS

#### PURPOSE:

AFTER STUDYING THE RELIABILITY OF THE ELECTRICAL CONNECTIONS, IT HAS BEEN DETERMINED THAT CONNECTOR POSITION ASSURANCE (CPA) RETAINERS ARE NO LONGER REQUIRED ON MANY OF THE ELECTRICAL CONNECTORS USED ON SATURN VEHICLES. THE FOLLOWING CONNECTORS STILL REQUIRE USE OF A CPA AND THE CPA'S WILL CONTINUE TO BE AVAILABLE THROUGH SATURN SERVICE PARTS.

CONNECTOR CONNECTOR DESCRIPTION P/N CPA P/N SIR ARMING SENSOR (3-WAY) 12126641 12052834 SIR ROLL CONNECTOR-IN-LINE (2-WAY) 12126598 12052834 SIR LEFT DISCRIMINATING SENSOR (3-WAY) 12126642 12052834 SIR RIGHT DISCRIMINATING SENSOR (2-WAY) 12126640 12052834 SIR RESISTOR MODULE (6-WAY) 12126595 12064989 SIR INFLATOR MODULE (2-WAY) NOT SERVICED 12077979 SC2 HEADLAMP MOTOR-INLINE (5-WAY) 12052600 12020833

FIGURES: 0

SATURN BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A SATURN RETAILER FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 SATURN CORPORATION U.S.A. ALL RIGHTS RESERVED.