SERVICE MANUAL UPDATE-BODY/ COLLISION REPAIR AND SPECS.. Saturn Saturn 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE-BODY/ COLLISION REPAIR AND SPECS.

#### SUBJECT: 1991-1992 Body/Collision Repair and Specifications Service Manual Updates (Revised Torque Specification for Door Hinge Bolts)

#### MODELS AFFECTED: All 1991 and 1992 Saturns

PURPOSE: The torque specification for the door hinge bolts, found on pages BDDR 34 and BDDR 49 under "Hinge Assembly" in the "1991-1992 Body/Collision Repair Service Manual" and page RFSP 70 of the "Revised 1991 - 1992 Specifications Service Manual" has been revised from 35 Nm (26 lbs. ft.) to 32 Nm (24 lbs. ft.). Please make these revisions to your copies of the "1991-1992 Body/Collision Repair Service Manual" and the "1991-1992 Revised Specifications Service Manual."

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.