INFORMATION ON SEAT BELT CLIP AVAILABILITY. Saturn Saturn 1992

For 1990-2009 cars

# INFORMATION ON SEAT BELT CLIP AVAILABILITY

#### SUBJECT: Information on Seat Belt Clip Availability

#### TO: Saturn Fixed Operation Managers

Saturn has released a seat belt clip (P/N 94844571) for use with the center rear lap belt on 1991-1994 Sedans and Wagons. Use of the seat belt clip will retain the lap belt adjustment, at a specific length, for convenience of repeated use. Retailers should advise customers of the proper installation and use of the seat belt clip.

#### PROCEDURE:

--------- 1. To properly adjust the center rear seat lap belt when using the seat belt clip, first insert the center latch plate into the buckle and pull on the lap belt's free end until the lap belt is snug.

#### NOTE: If installing a child restraint (child safety seat), be sure to route the lap belt through or around the child restraint, according to the child restraint manufacturer's instructions.

2. While holding the lap belt in its properly adjusted position, unbuckle the lap belt and place the seat belt clip onto the lap belt as shown in the illustration. Make sure both pieces of the lap belt webbing are held by the seat belt clip as shown.

3. With each use, briefly check the fit of the lap belt after it is buckled to be sure it is properly adjusted.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.