Use of Aftermarket Valve Spring Removal and Installation Tools. Saturn Saturn 1991

For 1990-2009 cars

# Use of Aftermarket Valve Spring Removal and Installation Tools

Subject: | Service Information on Use of Aftermarket Valve Spring Removal and Installation Tools

Models: | 1991 - 1995 Saturns

### Purpose

The use of aftermarket valve spring removal and installation tools may damage the valve stems on all Saturn engines and lifter bores on DOHC (LL0) engines. Saturn recommends the use of SA9124E, which is an essential tool, to remove and install valve springs on a Saturn vehicle.

Notice: All Engines - Damage to the valve stem may cut the valve stem oil seal assembly, resulting in oil consumption.

DOHC (LLO) Engines - Damage to the lifter bores may result, damage to the lifter assembly face (camshaft lobe contact surface) may occur. Refer to the illustration on the next page of this bulletin.