POPPING NOISE FROM DOOR CHECK LINKS (REPLACE CHECK LINKS). Saturn Saturn 1991

For 1990-2009 cars

# POPPING NOISE FROM DOOR CHECK LINKS (REPLACE CHECK LINKS)

#### SUBJECT: Popping Noise from Door Check Links (Replace Door Check Links with New Part) All 1991 Saturn Vehicles

CONDITION: Customer may experience a popping noise coming from door check links when opening and closing the doors.

CAUSE: Excessive clearance at check link pivot.

#### CORRECTIVE ACTION:

Replace door check links with new service parts, following the "Door Check Link" procedures located in the "Doors" section of the "Body Service Manual."

#### PARTS REQUIREMENTS:

21094826 Front Side Door Check Link Assembly (Sedan) 21094827 Rear Side Door Check Link Assembly (Sedan) 21094828 Front Side Door Check Link Assembly (Coupe)

#### LABOR OPERATION:

#### Claim Information:

To receive credit for this repair, submit a claim, as follows, for the doors which have check links replaced:

Case Labor Type Description Code Time ---- ---------------------------------- -------- ------- VW Replace Front Side Door Check Link B4070 RH 0.3 hrs Assembly (Sedan/Coupe) B4071 LH 0.3 hrs VW Replace Rear Side Door Check Link B4450 RH 0.3 hrs Assembly (Sedan) B4451 LH 0.3 hrs

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.