For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Steering Column Upper Trim Cover Tip Use gentle pressure to disengage the steering column upper trim cover.
2 | Steering Column Lower Trim Cover Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Steering Column Lower Trim Cover Tip Use gentle pressure to disengage the steering column lower trim cover.
4 | Steering Column Lower Trim Cover Screw Tighten 2.5 N·m (22 lb in)
5 | Steering Column Lower Trim Cover Tip Use gentle pressure to disengage the steering column lower trim cover.