For 1990-2009 cars
CTD Status: The scan tool displays the current arming status of the content theft system.
Current CTD Trigger: The scan tool displays the current input which has cause a content theft alarm.
Driver Identification: The scan tool displays the driver which has disarmed the content theft system.
Left Rear Door Ajar Switch : The scan tool displays the current status of the left rear door ajar switch.
Hood Closed Switch : The scan tool displays the status of the hood closed portion of the hood ajar switch.
Hood Open Switch: The scan tool displays the status of the hood open portion of the hood ajar switch.
Rear Closure Ajar Switch: The scan tool displays the current status of the rear closure ajar switch.
Right Rear Door Ajar Switch: The scan tool displays the current status of the right rear door ajar switch.
Theft LED: The scan tool displays the current status of the theft indicator as controlled by the content theft deterrent (CTD) system.