For 1990-2009 cars

Connector 1: | Battery Current Sensor
Connector 2: | Generator

### Battery Current Sensor

#### Connector Part Information

- OEM: 13519047
- Service: See Catalog
- Description: 3-Way F GT 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Battery Current Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK | 5076 | Current Sensor Supply Voltage
B | BN | 5077 | Current Sensor Low Reference
C | WH | 5075 | Seat Position Switch Low Reference

### Generator

#### Connector Part Information

- OEM: 12186308
- Service: 89046837
- Description: 2-Way F JPT, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Generator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 225 | Generator Turn On Signal
2 | GY | 23 | Generator Field Duty Cycle Signal