For 1990-2009 cars

### Removal Procedure

1. It is only necessary to lower the headliner. Only do those step in headliner replacement that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement .
2. Remove the front drain hose from the sunroof module.
3. Remove tape from the drain hose.
4. Remove the front drain hose from the retaining clips.
5. Pull the front drain hose out of the front hinge pillar.

### Installation Procedure

1. Push the drain hose into the hole in the front hinge pillar.
2. Connect the front drain hose to the retaining clips.
3. Connect the drain hose to the sunroof module.
4. Install the headliner. Refer to Headlining Trim Panel Replacement .