For 1990-2009 cars

Connector 1: | Ignition Lock Solenoid
Connector 2: | Ignition Switch

### Ignition Lock Solenoid

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ignition Lock Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1450 | --
B | PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control

### Ignition Switch

#### Connector Part Information

- OEM: HCMPBC06K
- Service: See Catalog
- Description: 6-Way F HCM Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Ignition Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 3 | Ignition 1 Voltage
2 | BN | 4 | Accessory Voltage
3 | RD/WH | 3340 | Battery Positive Voltage
4 | WH/BK | 1073 | Ignition Key Resistor Signal
5 | WH | 1390 | Off/Run/Crank Voltage
6 | -- | -- | Not Used