For 1990-2009 cars

Connector 1: | Amplifier C1 (U65)
Connector 2: | Amplifier C2 (U65)
Connector 3: | Amplifier C3 (U65)
Connector 4: | Audio/Video Adapter (UUC)
Connector 5: | Digital Radio Receiver (U2K)
Connector 6: | Infrared Transmitter Module (UUC)
Connector 7: | Noise Compensation Microphone (U3U)
Connector 8: | Radio C1
Connector 9: | Radio C2
Connector 10: | Radio C3 (UUC)
Connector 11: | Radio C4 (U3U)
Connector 12: | Speaker - LF
Connector 13: | Speaker - LF (Tweeter)
Connector 14: | Speaker - LR
Connector 15: | Speaker - RF
Connector 16: | Speaker - RF (Tweeter)
Connector 17: | Speaker - RR
Connector 18: | Speaker - Subwoofer (U65)
Connector 19: | Steering Wheel Control Switch - Right (UK3)
Connector 20: | Video Display (UUC)

### Amplifier C1 (U65)

#### Connector Part Information

- OEM: 6098-4713
- Service: 88988652
- Description: 8-Way F 2.8 Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 3, 4
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 5, 8
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Amplifier C1 (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-GN/BK | 1794 | Subwoofer Speaker Output (-)
2 | D-BU/WH | 346 | Subwoofer Speaker Output (+)
3 | D-GN | 1795 | Right Subwoofer Speaker Output (+)
4 | L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
5 | BK | 850 | Ground
6-7 | -- | -- | Not Used
8 | RD/WH | 2040 | Battery Positive Voltage

### Amplifier C2 (U65)

#### Connector Part Information

- OEM: 7283-5534-60
- Service: 89047090
- Description: 16-Way M YESC/USCAR Class II Sealed Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Amplifier C2 (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 116 | Left Rear Speaker Output (-)
2 | BN | 199 | Left Rear Speaker Output (+)
3 | D-BU | 46 | Right Rear Speaker Output (+)
4 | L-BU | 115 | Right Rear Speaker Output (-)
5-8 | -- | -- | Not Used
9 | D-GN | 117 | Right Front Speaker Output (-)
10 | L-GN | 200 | Right Front Speaker Output (+)
11 | TN | 201 | Left Front Speaker Output (+)
12 | GY | 118 | Left Front Speaker Output (-)
13-16 | -- | -- | Not Used

### Amplifier C3 (U65)

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F 0.64 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Amplifier C3 (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 1999 | Left Rear Low Level Audio Signal (-)
2 | TN | 1946 | Right Rear Low Level Audio Signal (-)
3 | BN/WH | 599 | Left Rear Low Level Audio Signal (+)
4 | D-BU | 546 | Right Rear Low Level Audio Signal (+)
5-7 | -- | -- | Not Used
8 | WH | 1487 | Antenna Enable Signal
9 | L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
10 | D-GN | 1947 | Left Front Low Level Audio Signal (-)
11 | L-GN | 1948 | Right Front Low Level Audio Signal (-)
12 | TN | 511 | Left Front Low Level Audio Signal (+)
13-15 | -- | -- | Not Used
16 | OG | 5748 | Radio Audio Mute Signal

### Audio/Video Adapter (UUC)

#### Connector Part Information

- OEM: 15480082
- Service: 19149303
- Description: 8-Way F Micro 64 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Audio/Video Adapter (UUC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BARE | 5345 | Drain Wire
2 | -- | -- | Not Used
3 | PU | 2056 | Auxiliary Video High Signal
4 | -- | -- | Not Used
5 | WH | 2058 | Auxiliary Audio Right Signal
6 | YE | 2059 | Auxiliary Audio Left Signal
7 | BARE | 5346 | Video Drain Wire
8 | -- | -- | Not Used

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM: 15394150
- Service: See Catalog
- Description: 16-Way F Micro 64 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN/WH | 372 | Remote Radio Audio Output (-)
2 | BN/WH | 367 | Remote Radio Left Audio Signal
3 | D-GN/WH | 368 | Remote Radio Right Audio Signal
4 | GY | 388 | Remote Radio Right Audio Signal
5 | D-GN | 5060 | Low Speed GMLAN Serial Data
6-8 | -- | -- | Not Used
9 | BK/WH | 651 | Ground
10 | -- | -- | Not Used
11 | BARE | 6759 | Discrete Audio Drain Wire
12-15 | -- | -- | Not Used
16 | RD/WH | 2340 | Battery Positive Voltage

### Infrared Transmitter Module (UUC)

#### Connector Part Information

- OEM: 15429806
- Service: See Catalog
- Description: 16-Way F Micro 64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Infrared Transmitter Module (UUC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 5826 | Left DVD Audio Signal (+)
2 | PU | 6979 | DVD Audio Common
3 | WH | 5828 | Right DVD Audio Signal (+)
4 | YE | 343 | Accessory Voltage
5-7 | -- | -- | Not Used
8 | OG/BK | 5831 | Remote Infra Red Signal (+)
9-11 | -- | -- | Not Used
12 | BK/WH | 1551 | Ground
13-15 | -- | -- | Not Used
16 | TN/WH | 5830 | Remote Infra Red Signal (-)

### Noise Compensation Microphone (U3U)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Noise Compensation Microphone (U3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | 655 | Cellular Microphone Signal
B | BARE | 1489 | Drain Wire

### Radio C1

#### Connector Part Information

- OEM: 7283-4490-30
- Service: 88988743
- Description: 14-Way F (BK)

#### Terminal Part Information

- Pins: 1, 8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 2, 3, 9, 10, 4, 5, 6, 6, 7, 13
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: Pins 2, 3, 9, 10 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 4, 5, 6, 6, 7, 13 - P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | 2040 | Battery Positive Voltage
2 | TN | 201 | Left Front Speaker Output (+)
3 | TN | 1875 | Right Front Speaker Output (+)
4 | GY | 655 | Cellular Microphone Signal (U3U)
5 | BARE | 1489 | Drain Wire (U3U)
6 | WH | 1487 | Antenna Enable Signal
7 | PU/WH | 1382 | LED Dimming Signal
8 | BK/WH | 1551 | Ground
9 | GY | 118 | Left Front Speaker Output (-)
10 | TN/WH | 1985 | 5-Volt Reference
11-12 | -- | -- | Not Used
13 | D-GN | 5060 | Low Speed GMLAN Serial Data
14 | -- | -- | Not Used

### Radio C2

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 8, 9, 10, 5, 5, 6, 6, 13, 13, 14, 14
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: Pins 1, 2, 8, 9, 10 - P/P
- Core/Insulation Crimp: Pins 5, 5, 6, 6, 13, 13, 14, 14 - See Terminal Repair Kit
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | 367 | Remote Radio Left Audio Signal (U2K)
2 | D-GN/WH | 368 | Remote Radio Right Audio Signal (U2K)
3-4 | -- | -- | Not Used
5 | BN | 199 | Left Rear Speaker Output (+)
6 | D-BU | 46 | Right Rear Speaker Output (+)
7 | -- | -- | Not Used
8 | OG | 5748 | Radio Audio Mute Signal (U65)
9 | TN/WH | 372 | Remote Radio Audio Output (-) (U2K)
10 | GY | 388 | Remote Radio Right Audio Signal (U2K)
11-12 | -- | -- | Not Used
13 | YE | 116 | Left Rear Speaker Output (-)
14 | L-BU | 115 | Right Rear Speaker Output (-)
15-16 | -- | -- | Not Used

### Radio C3 (UUC)

#### Connector Part Information

- OEM: 7283-9077-40
- Service: 89047195
- Description: 14-Way F Kaizen 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio C3 (UUC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 2059 | Auxiliary Audio Left Signal
2 | WH | 2058 | Auxiliary Audio Right Signal
3 | L-BU | 5826 | Left DVD Audio Signal (+)
4 | WH | 5828 | Right DVD Audio Signal (+)
5 | OG/BK | 5831 | Remote Infra Red Signal (+)
6 | PK/BK | 5844 | Video Bright Control
7 | D-GN | 6975 | DVD Video Signal (+)
8 | PU | 2056 | Auxiliary Video High Signal
9 | BARE | 5345 | Drain Wire
10 | BN/WH | 5846 | Video Power Mode Signal
11 | PU | 6979 | DVD Audio Common
12 | BARE | 6980 | DVD Audio Shield
13 | TN/WH | 5830 | Remote Infra Red Signal (-)
14 | BARE | 6976 | DVD Video Drain Wire
15 | WH/BK | 5335 | DVD Video Signal (-)
16 | BARE | 5346 | Video Drain Wire

### Radio C4 (U3U)

#### Connector Part Information

- OEM: 15394151
- Service: See Catalog
- Description: 16-Way F Micro 64 (BN)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio C4 (U3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | D-GN/WH | 817 | Vehicle Speed Signal (U3U)
6-16 | -- | -- | Not Used

### Speaker - LF

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - LF

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | TN | 201 | Left Front Speaker Output (+)

### Speaker - LF (Tweeter)

#### Connector Part Information

- OEM: 626064-0
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - LF (Tweeter)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | TN | 201 | Left Front Speaker Output (+)

### Speaker - LR

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - LR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 116 | Left Rear Speaker Output (-)
2 | BN | 199 | Left Rear Speaker Output (+)

### Speaker - RF

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - RF

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 117 | Right Front Speaker Output (-)
2 | TN | 200 | Right Front Speaker Output (+)

### Speaker - RF (Tweeter)

#### Connector Part Information

- OEM: 626064-0
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - RF (Tweeter)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 117 | Right Front Speaker Output (-)
2 | TN | 200 | Right Front Speaker Output (+)

### Speaker - RR

#### Connector Part Information

- OEM: 12196741
- Service: See Catalog
- Description: 2-Way F Faston 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - RR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 115 | Right Rear Speaker Output (-)
2 | BN | 46 | Right Rear Speaker Output (+)

### Speaker - Subwoofer (U65)

#### Connector Part Information

- OEM: 12064760
- Service: 12085208
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Subwoofer (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN/BK | 1794 | Subwoofer Speaker Output (-)
B | D-BU/WH | 346 | Subwoofer Speaker Output (+)
C | L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
D | D-GN | 1795 | Right Subwoofer Speaker Output (+)

### Steering Wheel Control Switch - Right (UK3)

#### Connector Part Information

- OEM: 31068-1010
- Service: See Catalog
- Description: 4-Way F HDAC64 SR Housing (BK)

#### Steering Wheel Control Switch - Right (UK3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 1450 | Ground
2 | PU/WH | 7005 | LED Dimming Signal
3 | PU | 1375 | Remote Radio Control Supply Voltage
4 | D-BU | 1796 | Steering Wheel Controls Signal

### Video Display (UUC)

#### Connector Part Information

- OEM: 7283-9088-30
- Service: See Catalog
- Description: 10-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Video Display (UUC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 6975 | DVD Video Signal (+)
2 | WH/BK | 5335 | DVD Video Signal (-)
3-5 | -- | -- | Not Used
6 | BK/WH | 1551 | Ground
7 | RD/WH | 2340 | Battery Positive Voltage
8 | WH | 1487 | Antenna Enable Signal
9 | PK/BK | 5844 | Video Bright Control
10 | BN/WH | 5846 | Video Power Mode Signal