For 1990-2009 cars

Name | AF33-5
--- | ---
RPO Codes | M09 or M45
Vehicle Platform Engine/Transmission Usage | L - SUV 3.6L LY7
Transmission Drive | FWD or AWD
1st Gear Ratio | 4.575
2nd Gear Ratio | 2.979
3rd Gear Ratio | 1.947
4th Gear Ratio | 1.318
5th Gear Ratio | 1.000
Reverse Ratio | 5.024
Pressure Taps | Line Pressure
Transmission Fluid Type | T - IV
Transmission Fluid Capacity - Approximate | Complete Overhaul: Dry 7.8L (8.2 qt)
Transmission Type: 5 | Five Forward Gears, Clutch to Clutch Shifting
Case Material | Die Cast Aluminum
Transmission Weight | 90 kg (198 lb)