For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GMLAN modules on this vehicle also support DTC Symptom information.

DTC | DTC Descriptor | Module that Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
Important: Do not clear any DTCs unless instructed to do so by a diagnostic procedure. Important: If any DTCs are Powertrain related DTCs, select Capture Info in order to store the DTC information with the scan tool. Diagnose any current DTCs in the following order:

1. DTCs that begin with a U
2. B1000, B1001, B1016, B1019, C0550, C0551, C0558, P0601, P0602, P0603, P0604, P0606, P2101, P2107, or P2610
3. B1325, B1424, B1517, C0800, C0899, C0900, P0560, P0562, or P0563
4. Component level DTCs
5. System level DTCs
6. Any remaining DTCs

B0000 | Vehicle Speed Information Circuit | Radio | DTC B0000
B0005 | In Park Switch Signal Circuit | BCM | DTC B0005
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0014 | Driver Side Frontal Deployment Loop | SDM | DTC B0014-B0045
B0015 | Driver Pretensioner Loop | SDM | DTC B0014-B0045
B0016 | Left Roof Rail Initiator 1 Deployment Loop | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0022 | Passenger Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0023 | Right Roof Rail Initiator 1 Deployment Loop | SDM | DTC B0014-B0045
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded With Loop DTCs Present | SDM | DTC B0052 or B0053
B0055 | Side Airbag Deployment Commanded | SDM | DTC B0055
B0056 | Passenger Frontal Airbag Suppressed | SDM | DTC B0056
B0057 | Passenger Side Airbag Suppressed | SDM | DTC B0057
B0058 | Passenger Pretensioner Suppressed | SDM | DTC B0058
B0073 | Passenger Seat Belt Sensor Circuit | SDM | DTC B0072 or B0073
B0081 | Passenger Presence System | SDM | DTC B0081
B0083 | Front End Sensor 1 | SDM | DTC B0083 or B0084
B0084 | Front End Sensor 2 | SDM | DTC B0083 or B0084
B0085 | Left Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0086 | Right Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0090 | Rollover Sensor | SDM | DTC B0090
B0158 | Outside Air Temperature Sensor Circuit | BCM | DTC B0158
B0228 | Recirculate Position Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0283 | Electric Rear Defrost Circuit | BCM | DTC B0283
B0413 | Temperature Control 1 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0423 | Temperature Control 2 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0433 | Temperature Control 3 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0835 | Cruise Control System Active Indicator Circuit | BCM | DTC B0835
B1000 | Electronic Control Unit (ECU) Performance | BCM, DRR, IPC, PPS, Radio, RCDLR, ROS, RSA, SDM, TDM, VCIM | DTC B1000
B1001 | Option Configuration Error | BCM, HVSM, PPS, Radio, ROS, SDM, VCIM | DTC B1001
SDM | DTC B1001
B1016 | VIN Not Programmed | BCM, TDM | DTC B1016
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | Left Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Right Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Left Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Right Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit | DRR | DTC B1259
B1287 | Amplifier Control Signal Circuit | Radio | DTC B1287
B1325 | Device Power Circuit | HVSM, IPC, PPS, Radio | DTC B1325
B1370 | Device Ignition 1 ON and START Circuit | BCM | DTC B1370
Device Ignition 1 Circuit | SDM | DTC B1370
B1380 | Device Ignition Accessory Circuit | BCM | DTC B1380
B1395 | Analog Reference Voltage | HSM | DTC B1395
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1428 | Ignition Switched Power Run/Crank Relay Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1441 | Device Ignition Off/Run/Crank Circuit | BCM | DTC B1441
B1475 | Retained Accessory Power Circuit | BCM | DTC B1475
B1516 | Battery Current Sensor Signal | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | High Parasitic Load Detected | BCM | DTC B1527
B1529 | Device Voltage Reference Output Circuit | BCM | DTC B1529
B1925 | Left Seat Cushion Heater Sensor Circuit | HSM | DTC B1925 or B2170
B2170 | Right Seat Cushion Heater Sensor Circuit | HSM | DTC B1925 or B2170
B2345 | Seat Heater Disable Circuit | HSM | DTC B2345
B2425 | Left Seat Heater Circuit | HSM | DTC B2425 or B2430
B2430 | Right Seat Heater Circuit | HSM | DTC B2425 or B2430
B2462 | Global Positioning System (GPS) | Navigation Radio | DTC B2462
B2474 | Navigation Display Head Backlighting Performance | Navigation Radio | DTC B2474
B2508 | Seat Heater Relay Circuit | HSM | DTC B2508 or B2509
B2530 | Front Fog Lamp Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2575 | Headlamp Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signal Mismatch | BCM | DTC B257A
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamp Control Circuit | BCM | DTC B2585
B2600 | Daytime Running Lamp Control Circuit | BCM | DTC B2600
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B2615 | Passenger Compartment Dimming 2 Circuit | BCM | DTC B2615
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2652 | Passenger Compartment Dimming 3 Circuit | BCM | DTC B2652
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2965 | Key In Ignition Circuit Open | BCM | DTC B2965
B3006 | Hood Ajar Circuit Plausibility Failure | BCM | DTC B3006
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109 | Keyless Entry Transmitter 1 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3110 | Keyless Entry Transmitter 2 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3111 | Keyless Entry Transmitter 3 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3112 | Keyless Entry Transmitter 4 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3445 | Stop Lamp Circuit | BCM | DTC B3445
B3600 | Passenger Compartment Dimming Request Signal Circuit | BCM | DTC B3600
B3622 | Steering Wheel Controls Signal Circuit | BCM | DTC B3622
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3779 | Air Flow Control 9 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B3782 | Air Flow Control 10 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3884 | Center High Mounted Stop Lamp (CHMSL) Circuit | BCM | DTC B3884
B3922 | Front Wiper Function Select Circuit | BCM | DTC B3922
B3933 | Evaporator Temperature Sensor Circuit | HVAC | DTC B3933
B3935 | Transponder Authentication Error | VTD | DTC B3935
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | ABS Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS) Brake Switch/Sensor Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0196 | Yaw Rate Circuit | EBCM | DTC C0196
C0201 | Antilock Brake System (ABS) Enable Relay Contact Circuit | EBCM | DTC C0201
C0252 | Steering Wheel Position Sensor Uncorrelated | EBCM | DTC C0252
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | EBCM | DTC C0277 or C0890
C0280 | Stability System Active Too Long | EBCM | DTC C0280
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0393 | Rear Axle Coupling Solenoid Control Circuit | CCM | DTC C0393
C0394 | Rear Axle Coupling Temperature Sensor Circuit | CCM | DTC C0394
C0460 | Steering Position Signal | EBCM | DTC C0460
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
TCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0558 | Calibration Mismatch | CCM | DTC C0558
C0561 | System Disabled Information Stored | EBCM | DTC C0561 or P0856
TCM | DTC C0561
C0750 | Left Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0775 | Low Tire Pressure System Sensors Not Learned | RCDLR | DTC C0775
C0890 | Device Voltage Reference Output 3 Circuit | BCM | DTC C0277 or C0890
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0036 | Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0102, or P0103
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0102, or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0102, or P0103
P0111 | Intake Air Temperature (IAT) Sensor Circuit Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0111-P0113
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0111-P0113
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0119
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0151
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0152
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153
P0134 | HO2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0134 or P0154
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0151 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151
P0152 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0157 | HO2S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0160 | HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0306
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0306
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0306
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0306
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0306
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0328 | Knock Sensor (KS) Circuit High Frequency Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) Circuit High Frequency Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Position (CKP) Sensor A Circuit | ECM | DTC P0335, P0336, or P0338
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0338
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338
P0341 | Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0346 | Intake Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0351 | Ignition Coil 1 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0352 | Ignition Coil 2 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0354 | Ignition Coil 4 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0355 | Ignition Coil 5 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0356 | Ignition Coil 6 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0391 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459
P0446 | Evaporative Emissions (EVAP) Vent System Performance | ECM | DTC P0446
P0449 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit | ECM | DTC P0449, P0498, or P0499
P0450 | Fuel Tank Pressure (FTP) Sensor Circuit | ECM | DTC P0450 or P0451
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0450 or P0451
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455 or P0497
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0481 | Cooling Fan Relay 2 and 3 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0496 | Evaporative Emission (EVAP) System Flow During Non-Purge | ECM | DTC P0496
P0497 | Evaporative Emission (EVAP) System No Flow During Purge | ECM | DTC P0455 or P0497
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Low Voltage | ECM | DTC P0449, P0498, or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit High Voltage | ECM | DTC P0449, P0498, or P0499
P0506 | Idle Speed Low | ECM | DTC P0506, P0507, or P050A
P0507 | Idle Speed High | ECM | DTC P0506, P0507, or P050A
P050A | Cold Start Idle Air Control (IAC) System Performance | ECM | DTC P0506, P0507, or P050A
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562 or P0563
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563
P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601-P0604, P0606, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601, P0602, P0603, or P0604
P0602 | Control Module Not Programmed | ECM | DTC P0601-P0604, P0606, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601, P0602, P0603, or P0604
P0603 | Control Module Long Term Memory Reset | ECM | DTC P0601-P0604, P0606, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601, P0602, P0603, or P0604
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601-P0604, P0606, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601, P0602, P0603, or P0604
P0606 | Control Module Internal Performance | ECM | DTC P0601-P0604, P0606, P062B, P0167D, P2107, or P2610
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0625 | Generator F-Terminal Circuit Low Voltage | ECM | DTC P0625
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629
P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P2100, P2101, or P2119
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0643 | 6-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0653 | 6-Volt Reference 2 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relays 2 and 3 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relays 2 and 3 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706-P0708
P0707 | Transmission Range (TR) Switch Circuit Low Voltage | TCM | DTC P0706-P0708
P0708 | Transmission Range (TR) Switch Circuit High Voltage | TCM | DTC P0706-P0708
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0730 | Incorrect Gear Ratio | TCM | DTC P0730
P0731 | Incorrect 1st Gear Ratio | TCM | DTC P0731
P0732 | Incorrect 2nd Gear Ratio | TCM | DTC P0732
P0733 | Incorrect 3rd Gear Ratio | TCM | DTC P0733
P0734 | Incorrect 4th Gear Ratio | TCM | DTC P0734
P0735 | Incorrect 5th Gear Ratio | TCM | DTC P0735
P0736 | Incorrect Reverse Ratio | TCM | DTC P0736
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742
P0762 | Shift Solenoid (SS) 3 Valve Performance - Stuck On | TCM | DTC P0762
P081A | Starter Inhibit Circuit Low Voltage | TCM | DTC P081A or P081B
P081B | Starter Inhibit Circuit High Voltage | TCM | DTC P081A or P081B
P0856 | Traction Control Request Circuit | ECM | DTC C0561 or P0856
P0864 | TCM Communication Circuit Performance | ECM | DTC P0864
P0897 | Transmission Fluid Life | TCM | DTC P0897
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0966 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0967 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0970 | Shift Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0971 | Shift Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0962, P0963, P0966, P0967, P0970, or P0971
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0979 | Shift Solenoid (SS) 3 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0980 | Shift Solenoid (SS) 3 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0982 | Shift Solenoid (SS) 4 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0983 | Shift Solenoid (SS) 4 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0985 | Shift Solenoid (SS) 5 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0986 | Shift Solenoid (SS) 5 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1719 | Incorrect Shifting Detected | TCM | DTC P1719
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2092 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2098
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 or P2099
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P2100, P2101, or P2119
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 2 | ECM | DTC P2232 or P2235
P2270 | HO2S Signal Stuck Lean Bank 1 Sensor 2 | ECM | DTC P2270 or P2272
P2271 | HO2S Signal Stuck Rich Bank 1 Sensor 2 | ECM | DTC P2271 or P2273
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534
P2536 | Ignition Accessory Switch Circuit | TCM | DTC P2536
P2636 | Fuel Transfer Pump Flow Insufficient | ECM | DTC P2636
P280A | Transmission Range (TR) Switch Circuit Not Learned | TCM | DTC P280A
U0073 | High Speed Communication Bus | BCM, DRR, HVSM, PPS, PSCM, Radio, RCDLR, ROS, RSA | DTC U0073 or U2100
U0100 | Lost Communication With Engine/Powertrain Control Module (ECM/PCM) | BCM, PSCM | DTC U0100-U0299
U0101 | Lost Communication With Transmission Control Module (TCM) | BCM | DTC U0100-U0299
U0102 | Lost Communication With Transfer Case Control Module | EBCM | DTC U0100-U0299
U0104 | Lost Communication With Cruise Control Module | BCM | DTC U0100-U0299
U0121 | Lost Communication With Electronic Brake Control Module (EBCM) | BCM | DTC U0100-U0299
U0122 | Lost Communication With Vehicle Dynamics Control Module | BCM | DTC U0100-U0299
U0131 | Lost Communication With Power Steering Control Module | BCM | DTC U0100-U0299
U0140 | Lost Communication With Body Control Module (BCM) | HVSM, PPS, PSCM, RCDLR, ROS, RSA, TDM | DTC U0100-U0299
U0151 | Lost Communication With Sensing and Diagnostic Module (SDM) | PPS, ROS | DTC U0100-U0299
U0155 | Lost Communication With Instrument Panel Cluster (IPC) Control Module | BCM, HVSM, PPS, RCDLR, ROS, RSA, TDM | DTC U0100-U0299
U0164 | Lost Communication With HVAC Control Module | BCM, HVSM | DTC U0100-U0299
U0168 | Lost Communication With Vehicle Theft Deterrent (VTD) Control Module | BCM | DTC U0100-U0299
U0170 | Lost Communication With Passenger Presence System (PPS) | SDM | DTC U0100-U0299
U0184 | Lost Communication With Radio | BCM, DRR, RSA | DTC U0100-U0299
U0198 | Lost Communication With Communication Interface Module (OnStar®) | BCM | DTC U0100-U0299
U0214 | Lost Communication With Remote Function Actuator (RFA) | BCM | DTC U0100-U0299
U1500 | Inter-Device Dedicated Bus 1 | EBCM, VCIM | DTC U1500
U1814 | Powertrain High Speed Communication Enable Circuit | BCM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2105 | Lost Communication With Engine Control System | EBCM | DTC U2105-U2199
U2106 | Lost Communications With Transmission Control System | EBCM | DTC U2105-U2199
U2107 | Lost Communications With Body Control System | EBCM | DTC U2105-U2199
U2142 | Lost Communication With Yaw Rate Sensor (YRS) | EBCM | DTC U2105-U2199
U2143 | Lost Communications With Steering Angle Sensor (SAS) | EBCM | DTC U2105-U2199