For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the rear brake shield. Refer to Rear Brake Shield Replacement.

1 | Park Brake Cable Eye

#### Procedure

1. Using the J 37043 , release the locking fingers on the park brake cable.
2. Remove the park brake cable from the actuator lever.

#### Special Tools

J 37043 Parking Brake Cable Release Tool

2 | Parking Brake Actuator

#### Procedure

Adjust the park brake. Refer to Park Brake Adjustment.