For 1990-2009 cars

## Liftgate Wedge Replacement Body Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement .

1 | Body Side Liftgate Wedge Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Body Side Liftgate Wedge

## Liftgate Wedge Replacement Liftgate Side

Callout | Component Name
--- | ---
1 | Liftgate Side Wedge Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Liftgate Side Wedge