For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
2. Lift up the rear of the front carpet retainer. Refer to Front Carpet Retainer Replacement .

1 | Center Pillar Lower Trim Panel Tip Start at the top of the lower garnish molding, pull at the clip locations to disengage the clips.
2 | Center Pillar Lower Trim Panel Retainer Clip (Qty: 5)