For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Auxiliary Temperature Actuator Screw | 2 N·m | 18 lb in
Auxiliary Mix Door Actuator Screw | 2 N·m | 18 lb in
Air Temperature Actuator to Evaporator Case Screws | 1.5 N·m | 13 lb in
HVAC Control to Center Trim Bezel Screws | 1.5 N·m | 13 lb in
Inside Air Temperature Sensor Screw | 2 N·m | 18 lb in
Liquid Line Nut to Condenser | 20 N·m | 15 lb ft
Mode Actuator to Evaporator Case Screws | 1.5 N·m | 13 lb in
Mode Cam Bracket to Evaporator Case Screws | 1.5 N·m | 13 lb in
Recirc Actuator to Air Inlet Screws | 1.5 N·m | 13 lb in