For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Body Side Liftgate Wedge Bolts | 10 N·m | 89 lb in
Front Door Check Link Bolts | 10 N·m | 89 lb in
Front Door Check Link Nuts | 10 N·m | 89 lb in
Front Fender Bolts | 10 N·m | 89 lb in
Front Side Door Hinge To Body Bolts | 31 N·m | 23 lb ft
Front Side Door Hinge To Door Bolts | 31 N·m | 23 lb ft
Fuel Filler Door Bolts | 2.5 N·m | 22 lb in
Hood Assist Rod Ball Stud Bolts | 10 N·m | 89 lb in
Hood Hinge Bolts | 25 N·m | 18 lb ft
Hood Primary Latch Striker | 25 N·m | 18 lb ft
Liftgate Hinge Bolts | 25 N·m | 18 lb ft
Liftgate Hinge Nuts | 25 N·m | 18 lb ft
Liftgate Side Wedge Bolts | 10 N·m | 89 lb in
Liftgate Strut Ball Stud Bolts | 10 N·m | 89 lb in
Primary Hood Latch Bolts | 10 N·m | 89 lb in
Rear Door Check Link Bolts | 10 N·m | 89 lb in
Rear Door Check Link Nuts | 10 N·m | 89 lb in
Rear Side Door Hinge To Body Bolts | 31 N·m | 23 lb ft
Rear Side Door Hinge To Door Bolts | 31 N·m | 23 lb ft
Secondary Hood Latch Bolts | 10 N·m | 89 lb in