For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. See Recommended Fluids and Lubricants for more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System

- Front Only Climate Control System

11.0 qt

10.4 L

- Front and Rear Climate Control System

12.0 qt

11.5 L

Engine Oil with Filter | 5.5 qt | 5.2 L
Fuel Tank | 18.5 gal | 70.0 L
Transmission Fluid | 4.1 qt | 3.9 L
Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

#### Engine Specifications

Engine | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
3.6L V6 | 7 | Automatic | 0.043 in (1.10 mm)