For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame Reinforcement Bolts | 50 N·m | 37 lb ft
Frame-To-Body Bolts | 155 N·m | 114 lb ft
Front Transaxle Mount Through Bolt | 110 N·m | 81 lb ft
Front Wheelhouse Liner Bolts | 10 N·m | 89 lb in
Front Wheelhouse Liner Screws | 6 N·m | 53 lb in
Rear Transaxle Mount-To-Frame Bolts | 50 N·m | 37 lb ft
Rear Wheelhouse Liner Panel Bolts | 10 N·m | 89 lb in
Rear Wheelhouse Liner Panel Nuts | 4 N·m | 35 lb in
Stabilizer Shaft Clamp Bolts | 50 N·m | 37 lb ft
Steering Gear Bolts | 110 N·m | 81 lb ft