For 1990-2009 cars

RPO | Description
--- | ---
APL | Seat Passenger - Delete
ATY | Seat Rear - Not Installed (Seat, Belts, Labels, Mounting Hardware)
AG1 | Adjuster Front Seat - Power, Multi-Directional, Driver
AL0 | Sensor Indicator - Inflatable Restraint, Front Passenger/Child Presence Detector
AM9 | Seat Rear - Not Installed (Seat, Belts, Labels, Mounting Hardware)
AP3 | Lock Control, Entry - Remote Entry, Do Not use after 2009 Model Year
AR9 | Seat - Front Bucket, Deluxe
AT8 | Restraint Provisions - Child, Rear Seat, Rear Facing
AU0 | Lock Control, Entry - Remote Entry, Do Not Use After 2009 Model Year
AY1 | Restraint System - Seat, Inflatable, Driver and Passenger, Roof Side
B1A | Plant Code - Ingersol, Ontario, Canada
CF5 | Roof - Sun, Glass, Sliding, Electric
CW7 | Country - Puerto Rico/US Virgin Island (Do Not Release Parts to This Option)
CV3 | Country - Mexico (Do Not Release Parts to This Option)
C4Y | GVW Rating - 2 425 kg (5,346 lbs)
C6B | GVW Rating - 2 475 kg (5,456 lbs)
C68 | HVAC System - Air Conditioner Front, Auto, Electronic Controls
C69 | HVAC System Rear - Air Conditioner
DD8 | Mirror Inside Rearview - Light Sensitive
DG7 | Mirror Outside - Left and Right, Remote Control, Electric, Color
FE1 | Suspension System - Soft Ride
FE9 | Certification - Emission, Federal
FR4 | Ratio - Transaxle Final Drive 2.48
IPB | Trim - Interior Design (PB)
IP2 | Trim - Interior Design (P2)
JL9 | Brake System - Power, Front and Rear Disc, Antilock, Front and Rear Wheel
KA1 | Heater - Seat, Front
KW7 | Generator - 170 Amp
KW8 | Generator - 155 Amp
K05 | Heater Engine - Block
K34 | Cruise Control - Automatic, Electronic
LY7 | Engine - Gas, 6 Cylinder, 3.6L, SFI, V6, Aluminum, 60 Degrees, GM
MX0 | Merchandised Trans - Auto Provisions, O/D
M09 | Transmission - Automatic 5 Speed, Aisin, AF33, (Tiptronic)
M45 | Transmission - Automatic 5 Speed, Opel, AF33, (Active Select)
NE1 | Certification - Emission, Geographically Restricted Registration For Vehicles Up To 14,000 lbs GVW (Use 2003 Model Year)
NK5 | Steering Wheel - Standard
NP5 | Steering Wheel - Leather Wrapped
NT7 | Emission System - Federal, Tier 2
NU5 | Emission System - California, BIN 4
N75 | Wheel - 17 x 7, Aluminum, Custom
PA2 | Wheel - 17 x 7, Aluminum, Chrome
PY0 | Wheel - 16 x 6.5, Aluminum
QKG | Tire All - P235/65R16-101S BW R/PE ST TL AL2
QLJ | Tire All - P235/60R17-100S BW R/PE ST TL AL2
QMU | Tire All - P235/60R17-100H BW TL AL3
TGN | Language Control - Spanish
T96 | Lamp - Fog, Front
UUC | Radio - AM/FM Stereo, Seek/Scan, CD, DVD, Auto Tone, Clock, ETR, MP3, RDS
UH8 | Cluster - Instrument, Cool Temp, Trip Odometer, Tach
UK3 | Control - Steering Wheel, Accessory
US8 | Radio - AM/FM Stereo, Seek/Scan, CD, Auto Tone, Clock, ETR, MP3, RDS
UW6 | Speaker System - 6, Custom
U1C | Radio - AM/FM Stereo, Seek/Scan, CD, Clock, ETR
U19 | Speedometer - Instrument, Kilometer and Miles, Kilometer Odometer
U2K | Digital Audio System - S-Band
U3U | Radio - AM/FM Stereo, Seek/Scan, DVD, CD, Clock, ETR, Navigation, Voice Recorder, MP3
U65 | Speaker System - 7, Premium
U80 | Display - Compass
VFF | Video Format - Region 1, NTSC
VFJ | Video Format - Region 2, PAL
VFM | Video Format - Region 4, NTSC
VH9 | Envelope - Owner Information Manual
VT7 | Owners Manual - English Language
VZ3 | Label - Mercury Disposal Notification
V1K | Bar - Luggage Carrier, Center Cross
V73 | Vehicle Statement - USA/Canada
V78 | Vehicle Statement - Delete
YB6 | Axle - (Base Equipment) (Keep as Processing Option)
YF5 | Certification - Emission, California
Z49 | Export - Canadian Modified Mandatory Base Equipment
1SA | Package - Option 01
1SB | Package - Option 02
1SC | Package - Option 03
1SD | Package - Option 04
1SE | Package - Option 05
1SF | Package - Option 06
1SG | Package - Option 07
1SH | Package - Option 08
1SJ | Package - Option 09