For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Lower Control Arm Bolt | 160 N·m | 118 lb ft
Lower Control Arm to Support Assembly Bolt | 110 N·m | 81 lb ft
Lower Shock Absorber Bolt | 110 N·m | 81 lb ft
Rear Brake Hose Bracket Nut/Bolt | 12 N·m | 106 lb in
Spring Jounce Bumper | 480° from the intial contact ± 60° | 480° from the intial contact ± 60°
Stabilizer Link to Lower Control Arm Nut | 15 N·m | 11 lb ft
Stabilizer Link to Stabilizer Shaft Nut | 50 N·m | 37 lb ft
Stabilizer Shaft Clamp Bolt | 70 N·m | 52 lb ft
Toe Link Bolt | 160 N·m | 118 lb ft
Toe Link to Knuckle Bolt | 160 N·m | 118 lb ft
Toe Link to Support Bolt | 160 N·m | 118 lb ft
Trailing Arm Bolt | 110 N·m | 81 lb ft
Trailing Arm Bracket to Body Bolt | 110 N·m | 81 lb ft
Trailing Arm Bracket to Knuckle Bolt | 110 N·m | 81 lb ft
Trailing Arm Bushing Bolt | 160 N·m | 118 lb ft
Upper Control Arm to Knuckle Bolt | 160 N·m | 118 lb ft
Upper Control Arm to Support Bolt | 164 N·m | 121 lb ft
Upper Shock Bolt | 110 N·m | 81 lb ft
Wheel Bearing/Hub Bolt | 75 N·m | 55 lb ft
Wheel Drive Shaft Nut - AWD | 205 N·m | 151 lb ft