For 1990-2009 cars

Connector 1: | Seat Belt Switch - Left
Connector 2: | Seat Belt Switch - Right

### Seat Belt Switch - Left

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Switch - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN | 5016 | Seat Belt Switch - Left - Signal (w/o AG1)
D-BU | 5016 | Seat Belt Switch - Left - Signal (w/AG1)
B | PK | 5057 | Seat Position Sensor - Low Reference (w/o AG1)
TN/WH | 5057 | Seat Position Sensor - Low Reference (w/AG1)

### Seat Belt Switch - Right

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Switch - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN | 5057 | Seat Position Sensor - Low Reference
B | RD | 1362 | Seat Belt Switch - Right - Signal