For 1990-2009 cars

#### Body Control Module

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Door Lock Test | Driver Door Unlock | The BCM actuates the driver door unlock relay when you select UNLOCK. The driver door should unlock. The BCM actuates the door lock relay when you select LOCK. All doors and liftgate should lock.
Door Lock Test | Passenger Door Unlock | The BCM actuates the door unlock relay when you select UNLOCK. All passenger doors and liftgate should unlock. The BCM actuates the door lock relay when you select LOCK. All doors and liftgate should lock.