For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement

1 | Radio Screw (Qty: 4) Tighten 2 N·m (18 lb in)
2 | Radio Assembly

#### Procedure

1. Disconnect the antenna and electrical connectors from the rear of the radio.
2. Reprogram the radio after replacement. Refer to Control Module References