For 1990-2009 cars

### Display Screen

The rear display screen shows video from either DVD movies, or an AUX input device, such as a video game console or camera. Each video screen has a dedicated video signal circuit to the radio.

### AUX Inputs

The AUX input jacks are standard color-coded RCA-style jacks. Video is yellow, right audio is red, and left audio is white. The jacks are located on the rear of the center console. A number of devices may be plugged into the AUX jacks, including, but not limited to video game consoles, digital cameras, camcorders, or other devices. Audio only sources can be played through the AUX jacks from portable audio devices.

### Rear Seat Entertainment (RSE)

The rear seat entertainment (RSE) system includes a radio with a DVD player, a video display screen, 2 wireless headphones, and a remote control. The rear video display receives a video signal directly from the radio. The infrared transmitter located on the overhead console receives video or AUX audio directly from the radio and then is transmitted to the wireless headphones.

### Wireless Headphones

Wireless headphones are optional and allow for rear seat passengers to use the rear seat entertainment (RSE) functions without disturbing the listening of front seat passengers. The wireless headphones receive audio signals from an infrared transmitter on the overhead console. This transmission is line of sight only, so audio quality will be degraded if anything blocks the transmitter signal from reaching the headphones.

To use wireless headphones, turn them on using the power button on the left side headphone earpiece. Adjust volume using the rotary dial on the right side headphone earpiece.