For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter to Exhaust Flexible Pipe Nut | 22 N·m | 16 lb ft
Catalytic Converter to Exhaust Manifold Nut | 50 N·m | 37 lb ft
Catalytic Converter Nut | 50 N·m | 37 lb ft
Dash Panel Heat Shield | 10 N·m | 89 lb in
Exhaust Manifold Bolt | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Muffler Clamp | 5 N·m | 44 lb in
Fuel Tank Strap Bolt | 25 N·m | 18 lb ft
Rear Exhaust Manifold Heat Shield Bolt | 50 N·m | 37 lb ft