For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ground Terminal Nut | 9 N·m | 80 lb
Power Steering Cooler Pipe Fitting | 25 N·m | 18 lb ft
Power Steering Gear Bolt | 110 N·m | 81 lb ft
Power Steering Gear Hoses Bracket Bolt | 9 N·m | 80 lb in
Power Steering Gear Inlet Hose Fitting | 25 N·m | 18 lb ft
Power Steering Pump Bolt | 50 N·m | 37 lb ft
Power Steering Pump Inlet Pipe Bolt | 8 N·m | 71 lb in
Rack And Pinion Outer Tie Rod End Nut | 25 N·m plus 90 degrees | 18 lb ft plus 90 degrees
Remote Power Steering Fluid Reservoir Bolt | 9 N·m | 80 lb in
Remote Power Steering Fluid Reservoir Stud | 9 N·m | 80 lb in
Steering Gear Pipe Fitting | 25 N·m | 18 lb ft
Steering Gear Inner Tie Rod | 78 N·m | 58 lb ft
Transaxle Mount Bolt | 50 N·m | 37 lb ft
Transaxle Mount Bolt | 110 N·m | 81 lb ft