For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter Housing Outer Seal
2 | Torque Converter and Support and A/Trans Fluid Pump Housing Assembly
3 | Torque Converter and Differential Housing Bolts M8 x 35 (Qty: 17) Caution: Some bolt torques specifications are different. Over tightening the bolts at the 12, 15 and 17 positions in the sequence could cause damage to the case threads. Caution: Refer to Fastener Caution in the Preface section.

#### Procedure:

Tighten in sequence shown.

Tighten

• | Bolts 1-11, 13-14 and 16 to 36N·m (27 lb ft)

• | Bolts 12, 15 and 17 to 30 N·m (22 lb ft)